;; netrtwlanu.inf 
;;
;; Realtek Wireless 802.11b/g/n USB 2.0 Network Adapter
;;
;; Copyright (C) 2012 Realtek Semiconductor Corp.
;;
;; This release is primarily for WHQL test.
;;

;; FOR XP/Vista/Win7/Win8

[Version]
Signature	= "$Windows NT$"
Class		= Net
ClassGUID	= {4d36e972-e325-11ce-bfc1-08002be10318}
Provider	= %Realtek%
CatalogFile.NT	= netrtwlanu.cat		;; for WHQL certified
DriverVer = 12/16/2014,1027.3.1015.2014

[Manufacturer]
%Realtek% = Realtek,NTamd64.6.2
%PCI% = PCI,NTamd64.6.2
%Sitecom% = Sitecom,NTamd64.6.2
%EDIMAX% = EDIMAX,NTamd64.6.2
%Abocom% = Abocom,NTamd64.6.2
%Amigo% = Amigo,NTamd64.6.2
%Hercules% = Hercules,NTamd64.6.2
%DLink% = DLink,NTamd64.6.2
%Belkin% = Belkin,NTamd64.6.2
%Zyxel% = Zyxel,NTamd64.6.2
%ATKK% = ATKK,NTamd64.6.2
%TRENDnet% = TRENDnet,NTamd64.6.2
%Feixun% = Feixun,NTamd64.6.2
%NetweeN% = NetweeN,NTamd64.6.2
%XAVI% = XAVI,NTamd64.6.2
%Netgear% = Netgear,NTamd64.6.2
%Oar_Inc% = Oar_Inc,NTamd64.6.2
%ASUS% = ASUS,NTamd64.6.2
%HAWKING% = HAWKING,NTamd64.6.2
%Compare% = Compare,NTamd64.6.2
%IO_DATA% = IO_DATA,NTamd64.6.2
%TPLINK% = TPLINK,NTamd64.6.2
%Logitec% = Logitec,NTamd64.6.2
%NEC% = NEC,NTamd64.6.2
%WD% = WD,NTamd64.6.2
%EnGenius% = EnGenius,NTamd64.6.2
%Linksys% = Linksys,NTamd64.6.2
%ACTIONTEC% = ACTIONTEC,NTamd64.6.2
%BUFFALO% = BUFFALO,NTamd64.6.2
%ELECOM% = ELECOM,NTamd64.6.2
%Amped% = Amped,NTamd64.6.2
%Qihoo% = Qihoo,NTamd64.6.2

[ControlFlags]
ExcludeFromSelect = *

[Realtek.NTamd64.6.2]
;; For 8192C RTK common		================================================================
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BFF&PID_8160								; RTK 88CU board for B/G/N      
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176								; RTK 88CU board for B/G/N
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8176&REV_0200&SS
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177							; RTK 88CU board for B/G
%RTL8188cu_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_8177&REV_0200&SS
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170							; RTK 88CE_VAU board for B/G/N
%RTL8188ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8170&REV_0200&SS
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E						; RTK 88CE_VAU board for B/G
%RTL8188ce_vau_G.DeviceDesc% 		= RTL8192cu_G.ndi, 		USB\VID_0BDA&PID_817E&REV_0200&SS
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C							; RTK 92CE_VAU board for B/G/N
%RTL8192ce_vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817C&REV_0200&SS
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A						; RTK slim_solo board for B/G/N
%RTL8188cu_slim_solo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817A&REV_0200&SS
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A					; LC slim solo for BGN.
%RTL8188cu_slim_solo_lc.DeviceDesc% = RTL8192cu_wow.ndi, 	USB\VID_0BDA&PID_819A&REV_0200&SS
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B					; RTK slim_combo board for B/G/N
%RTL8188cu_slim_combo.DeviceDesc% 	= RTL8192cu.ndi, 		USB\VID_0BDA&PID_817B&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu8188RU.ndi,USB\VID_0BDA&PID_817F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu8188RU.ndi,USB\VID_0BDA&PID_817F&REV_0200&SS
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F								; RTK 88RU board for B/G/N
%RTL8188ru.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_317F&REV_0200&SS
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A								; RTK 88RU board for B/G/N
%RTL8188cus_vl.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_818A&REV_0200&SS
%RTL8188cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_103C&PID_1629								; HP/Liteon board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8192
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178								; RTK 92CU board for B/G/N
%RTL8192cu.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0BDA&PID_8178&REV_0200&SS
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358								; AZ 88CE_VAU for B/G/N
%RTK_AZ88vau.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3358&REV_0200&SS
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359							; AZ 88CE_VAU for B/G
%RTK_AZ88vau_G.DeviceDesc% 			= RTL8192cu_G.ndi, 		USB\VID_13D3&PID_3359&REV_0200&SS
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357								; AZ 88CUS for B/G/N
%RTK_AZ88cus.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_13D3&PID_3357&REV_0200&SS
%RTL8188ctv.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0BDA&PID_018A								; 8188CTV for BGN test only.

;; For 8192D RTK common		================================================================
%RTL8192du.DeviceDesc% 				= RTL8192du.ndi, 	USB\VID_0BDA&PID_8194
%RTL8192du.DeviceDesc%  			= RTL8192du.ndi, 	USB\VID_0BDA&PID_8111
%RTL8192du0.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_8193&MI_00
%RTL8192du1.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_8193&MI_01
%RTL8192du2.DeviceDesc% 			= RTL8192du0.ndi, 	USB\VID_0BDA&PID_0193&MI_00
%RTL8192du3.DeviceDesc% 			= RTL8192du1.ndi, 	USB\VID_0BDA&PID_0193&MI_01

;; For 8723 RTK common		================================================================
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_872B
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_8725&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0723&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_0724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&MI_02
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_1724&REV_0200&MI_02&SS
%RTL8723au.DeviceDesc%  			= RTL8723au.ndi, 	USB\VID_0BDA&PID_A724

;; For 8188E RTK common		================================================================
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179
%RTL8188eu.DeviceDesc%  			= RTL8188eu.ndi, 	USB\VID_0BDA&PID_8179&REV_0200&SS
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179
%RTL8188ee_vau.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_A179&REV_0200&SS
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179
%RTL8188eu_0179.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_0BDA&PID_0179&REV_0200&SS

;; For 8812A RTK common		================================================================
%RTL8812au.DeviceDesc% 				= RTL8812au.ndi, 	USB\VID_0BDA&PID_8812
%RTL8812au_881A.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881A
%RTL8812au_881B.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881B
%RTL8812au_881C.DeviceDesc% 		= RTL8812au_Vx.ndi, USB\VID_0BDA&PID_881C

;; For 8811A RTK common		================================================================
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 	USB\VID_0BDA&PID_0811
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 	USB\VID_0BDA&PID_A811
%RTL8811au.DeviceDesc% 					= RTL8811au.ndi, 	USB\VID_7392&PID_A813
%RTL8811au_Combo.DeviceDesc% 			= RTL8821auLC.ndi, 	USB\VID_0BDA&PID_0823&MI_02

;; For 8192E RTK common		================================================================
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818B
%RTL8192eu.DeviceDesc% 				= RTL8192eu.ndi, 	USB\VID_0BDA&PID_818C&MI_02

;; For 8821B RTK common		================================================================
%RTL8821bu.DeviceDesc% 				= RTL8821bu.ndi, 	USB\VID_0BDA&PID_B821
%RTL8821bu.DeviceDesc% 				= RTL8821bu.ndi, 	USB\VID_0BDA&PID_B82B

;;----------------------------------------------------------------------------
;; For 8814A RTK common
;;----------------------------------------------------------------------------
%RTL8814au.DeviceDesc% 				= RTL8814au.ndi, 	USB\VID_0BDA&PID_8813

;;----------------------------------------------------------------------------
;; For 8723B RTK common
;;----------------------------------------------------------------------------
%RTL8723bu.DeviceDesc% 				= RTL8723bu.ndi, 	USB\VID_0BDA&PID_B720&MI_02

[PCI.NTamd64.6.2]
;; For 8192C PCI			================================================================
%PCI.DeviceDesc% 					= RTL8192cu.ndi, 	USB\VID_2019&PID_ED17
%PCI-2.DeviceDesc% 					= RTL8192cu.ndi, 	USB\VID_2019&PID_4902
%PCI_Abocom88cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_2019&PID_AB2A
%PCI_Abocom92cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_2019&PID_AB2B
%PCI_Vencer.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2019&PID_1201

;; For 8192D PCI			================================================================
%PCI_Abocom_du0.DeviceDesc% 		= RTL8192du0.ndi,	USB\VID_2019&PID_AB2C&MI_00
%PCI_Abocom_du1.DeviceDesc% 		= RTL8192du1.ndi,	USB\VID_2019&PID_AB2C&MI_01
%PCI_3_du0.DeviceDesc% 				= RTL8192du0.ndi,	USB\VID_2019&PID_4903&MI_00
%PCI_3_du1.DeviceDesc% 				= RTL8192du1.ndi,	USB\VID_2019&PID_4903&MI_01
%PCI_4_du0.DeviceDesc% 				= RTL8192du0.ndi,	USB\VID_2019&PID_4904&MI_00
%PCI_4_du1.DeviceDesc% 				= RTL8192du1.ndi,	USB\VID_2019&PID_4904&MI_01
%PCIWIDI_92DU.DeviceDesc% 			= RTL8192du.ndi, 	USB\VID_2019&PID_AB2D

;; For 8812A ABOCOM			================================================================
%PCI_AB30.DeviceDesc% 		= RTL8812au.ndi, 	USB\VID_2019&PID_AB30

;; For 8811A ABOCOM			================================================================
%PCI_AB32.DeviceDesc% 		= RTL8811au_PCI.ndi, 	USB\VID_2019&PID_AB32

[Sitecom.NTamd64.6.2]
;; For 8192C SITECOM			================================================================
%Sitecom.DeviceDesc% 				= RTL8192cu.ndi, USB\VID_0DF6&PID_0052
%Sitecom_UN.DeviceDesc% 			= RTL8192cu.ndi, USB\VID_0DF6&PID_005C
%Sitecom_HG.DeviceDesc% 			= RTL8192cu.ndi, USB\VID_0DF6&PID_0061
;; For 8812A Sitecom			================================================================
%Sitecom_0074.DeviceDesc% 			= RTL8812au.ndi, USB\VID_0DF6&PID_0074
;; For 8811A Sitecom			================================================================
%Sitecom_007A.DeviceDesc% 			= RTL8811au.ndi, USB\VID_0DF6&PID_007A

[EDIMAX.NTamd64.6.2]
;; For 8192C EDIMAX			================================================================
%EDIMAX.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_7392&PID_7811
%EDIMAX300.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_7392&PID_7822
;; For 8812A Edimax			================================================================
%Edimax_A822.DeviceDesc% 		= RTL8812au.ndi, 	USB\VID_7392&PID_A822
;; For 8811A Edimax			================================================================
%Edimax_AC600.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_7392&PID_A811
%Edimax_AC600.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_7392&PID_A812
;; For 8192D EDIMAX			================================================================
%EDIMAX5G.DeviceDesc% 			= RTL8192du_5G.ndi, 	USB\VID_0BDA&PID_E194

[ELECOM.NTamd64.6.2]
;; For 8192C ELECOM			================================================================
%ELECOM_4009.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_056E&PID_4009
;; For 8188E ELECOM			================================================================
%ELECOM_4008.DeviceDesc% 				= RTL8188eu.ndi, 		USB\VID_056E&PID_4008
;; For 8811A ELECOM			================================================================
%ELECOM_WDC433DU2.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_056E&PID_4007

[Abocom.NTamd64.6.2]
;; For 8192C ABOCOM			================================================================
%Abocom.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_07B8&PID_8189
%Abocom92cu.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_07B8&PID_8178

;; For 8192D ABOCOM			================================================================
%Abocom_92DU0.DeviceDesc% 		= RTL8192du0.ndi, 	USB\VID_07B8&PID_8193&MI_00
%Abocom_92DU1.DeviceDesc% 		= RTL8192du1.ndi, 	USB\VID_07B8&PID_8193&MI_01

;; For 8192E ABOCOM			================================================================
%Abocom_AB33.DeviceDesc% 		= RTL8192eu.ndi, 	USB\VID_2019&PID_AB33

;; For 8188E ABOCOM			================================================================
%Abocom_8179.DeviceDesc% 		= RTL8188eu.ndi, 	USB\VID_07B8&PID_8179

;; For 8812A ABOCOM			================================================================
%Abocom_8812.DeviceDesc% 		= RTL8812au.ndi, 	USB\VID_07B8&PID_8812

;; For 8811A ABOCOM			================================================================
%Abocom_0811.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_07B8&PID_0811

[Amigo.NTamd64.6.2]
;; For 8192C AMIGO			================================================================
%Amigo.DeviceDesc% 				= RTL8192cu.ndi, 	USB\VID_0EB0&PID_9071

[Hercules.NTamd64.6.2]
;; For 8192C HERCULES		================================================================
%Hercules.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_06F8&PID_E033
%Hercules-E035.DeviceDesc% 		= RTL8192cu.ndi, 	USB\VID_06F8&PID_E035

[DLink.NTamd64.6.2]
;; For 8192C DLINK			================================================================
%DLink-1.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_330A
%DLink-2.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3309
%DLink-3.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3308
%DLink-4.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_3307
%DLink-5.DeviceDesc% 			= RTL8192cu.ndi, 	USB\VID_2001&PID_330B

%DLink-DWA151.DeviceDesc% 		= RTL8192du.ndi, 	USB\VID_2001&PID_330C


%DLink_2001.DeviceDesc% 		= RTL8192eu.ndi, 	USB\VID_3312&PID_2001

;; For 8188E RTK common		================================================================
%DLINK_330F.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_2001&PID_330F
%DLINK_3310.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_2001&PID_3310
%DLINK_3311.DeviceDesc%  		= RTL8188eu.ndi, 	USB\VID_2001&PID_3311

;; For 8812A DLINK			================================================================
%DLink-DWA183.DeviceDesc% 			= RTL8812auDLink.ndi, 	USB\VID_2001&PID_330E
%DLink-DWA182.DeviceDesc% 			= RTL8812auDLink.ndi, 	USB\VID_2001&PID_3313
%DLink_3315.DeviceDesc% 			= RTL8812auDLink.ndi, 	USB\VID_2001&PID_3315
%DLink_3316.DeviceDesc% 			= RTL8812auDLink.ndi, 	USB\VID_2001&PID_3316

;; For 8811A DLINK			================================================================
%DLink-DWA171.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_2001&PID_3314
%DLink_3318.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_2001&PID_3318

[Belkin.NTamd64.6.2]
;; For 8192C BELKIN			================================================================
%Belkin.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_1102
%Belkin-2.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_2102
%Belkin-3.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_2103
%Belkin-4.DeviceDesc% 			= Belkin.ndi, 		USB\VID_050D&PID_1004

;; For 8192D BELKIN			================================================================
%Belkin-N600DB.DeviceDesc% 		= BelkinN600.ndi, 	USB\VID_050D&PID_110A
%Belkin-N450DB.DeviceDesc% 		= BelkinN450.ndi, 	USB\VID_050D&PID_1105
%Belkin-N300DB.DeviceDesc% 		= BelkinN300.ndi, 	USB\VID_050D&PID_120A 

;; For 8812A BELKIN			================================================================
%Belkin-AC950.DeviceDesc% 			= RTL8812auBelkin.ndi, 	USB\VID_050D&PID_1109

[BUFFALO.NTamd64.6.2]
;; For 8811A BUFFALO			================================================================
%Buffalo-WI-U2-433DM.DeviceDesc% 	= RTL8811au.ndi, 		USB\VID_0411&PID_0242	;For Buffalo WI-U2-433DM

;; For 8812A BUFFALO			================================================================
%Buffalo_025D.DeviceDesc% 	= RTL8812au.ndi, 		USB\VID_0411&PID_025D	;For Buffalo WI-U3-866D

[Zyxel.NTamd64.6.2]
;; For 8192C ZYXEL			================================================================
%Zyxel.DeviceDesc% 				= RTL8192cu.ndi, 	USB\VID_0586&PID_341F
;; For 8812A Zyxel			================================================================
%Zyxel_3426.DeviceDesc% 		= RTL8812au.ndi, 	USB\VID_0586&PID_3426

[ATKK.NTamd64.6.2]
;; For 8192C ATKK			================================================================
%ATKK.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_07AA&PID_0056

[TRENDnet.NTamd64.6.2]
;; For 8192C TREDENT			================================================================
%TRENDnet.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_20F4&PID_648B
%TRENDnet_2.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_20F4&PID_624D

;; For 8192D TREDENT			================================================================
%TRENDnet_3_du.DeviceDesc%		= RTL8192du.ndi, 		USB\VID_20F4&PID_664B

;; For 8812 TREDENT			================================================================
%TRENDnet_805B.DeviceDesc%		= RTL8812au.ndi, 		USB\VID_20F4&PID_805B

;; For 8811A Trendnet	================================================================
%TRENDnet_804B.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_20F4&PID_804B

[Feixun.NTamd64.6.2]
;; For 8192C FEXIUN			================================================================
%Feixun.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4855&PID_0090				; Feixun 88CUS for B/G/N
%Feixun.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4855&PID_0091				; Feixun 92CU for B/G/N

[NetweeN.NTamd64.6.2]
;; For 8192C NETWEEN			================================================================
%NetweeN.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_4856&PID_0091			; Feixun 8188CUS for B/G/N

[XAVI.NTamd64.6.2]
;; For 8192C XAVI			================================================================
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF7				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF9				; XAVI 88CUSlim solo for B/G/N
%XAVI.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFA				; XAVI 88CUSlim solo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFF8				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFB				; XAVI 88CUSlim combo for B/G/N
%XAVI88cusc.DeviceDesc% 		= RTL8192cu.ndi, 		USB\VID_04F2&PID_AFFC				; XAVI 88CUSlim combo for B/G/N

[Netgear.NTamd64.6.2]
;; For 8192C NETGEAR			================================================================
;;%Netgear.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0846&PID_9041				; Netgear 88CUSfor B/G/N

;; For 8812A Netgear			================================================================
;;%Netgear-A6200v2.DeviceDesc% 		= RTL8812au.ndi, 		USB\VID_0846&PID_9051

;; For 8811A Netgear			================================================================

[Oar_Inc.NTamd64.6.2]
;; For 8192C OAR			================================================================
%Oar_Inc.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_2019&PID_AB2E

[ASUS.NTamd64.6.2]
;; For 8192C ASUS			================================================================
%ASUS.DeviceDesc% 				= RTL8192cu.ndi, 		USB\VID_0B05&PID_17AB
%ASUS-2.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0B05&PID_17BA
%ASUS-17C0.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0B05&PID_17C0

;; For 8812A ASUS			================================================================
%ASUS_17D2.DeviceDesc% 			= RTL8812auASUS.ndi, 		USB\VID_0B05&PID_17D2

[HAWKING.NTamd64.6.2]
;; For 8192C HAWKING			================================================================
%Hawking-1.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0E66&PID_0019
%Hawking-2.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_0E66&PID_0020

;; For 8812A ASUS			================================================================
%Hawking_0022.DeviceDesc% 		= RTL8812au.ndi, 		USB\VID_0E66&PID_0022

;; For 8811A Hawking		================================================================
%Hawking_0023.DeviceDesc% 		= RTL8811au.ndi, 		USB\VID_0E66&PID_0023

[Compare.NTamd64.6.2]
;; For 8192C COMPARE			================================================================
%Compare-1.DeviceDesc% 			= RTL8192cu.ndi, 		USB\VID_CDAB&PID_8010

[IO_DATA.NTamd64.6.2]
;; For 8192C IO_DATA			================================================================
%IO_DATA_094c.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_04BB&PID_094C
%IO_DATA_0950.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_04BB&PID_0950

;; For 8812A IO_DATA			================================================================
%IO_DATA_0952.DeviceDesc% 		= RTL8812au.ndi, USB\VID_04BB&PID_0952

;; For 8811A IO_DATA			================================================================
%IO_DATA_AC433UA.DeviceDesc% 		= RTL8811au.ndi, 	USB\VID_04BB&PID_0953
%IO_DATA_0959.DeviceDesc% 		= RTL8811au_IO_DATA.ndi, 	USB\VID_04BB&PID_0959

[TPLINK.NTamd64.6.2]
;; For 8192C TPLINK			================================================================
%TPLINK-0100.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_2357&PID_0100

;; For 8812A TPLINK			================================================================
%TPLINK_0101.DeviceDesc% 		= RTL8812autplink.ndi, USB\VID_2357&PID_0101


[Logitec.NTamd64.6.2]
;; For 8192C Logitec			================================================================
%Logitec_016D.DeviceDesc% 		= RTL8192cu.ndi, USB\VID_0789&PID_016D
;; For 8192D Logitec			================================================================
%Logitec.DeviceDesc%			= RTL8192du_5G.ndi, 		USB\VID_0789&PID_0019

;; For 8812A Logitec			================================================================
%Logitec_016E.DeviceDesc% 		= RTL8812au.ndi, USB\VID_0789&PID_016E

[NEC.NTamd64.6.2]
;; For 8812A NEC			================================================================
%NEC_0408.DeviceDesc%			= RTL8812auNEC.ndi, USB\VID_0409&PID_0408

[WD.NTamd64.6.2]
;; For 8812A WD				================================================================
%WD_0632.DeviceDesc%			= RTL8812au.ndi, USB\VID_1058&PID_0632

[EnGenius.NTamd64.6.2]
;; For 8812A EnGenius			================================================================
%EnGenius_0100.DeviceDesc%		= RTL8812au.ndi, USB\VID_1740&PID_0100

[Linksys.NTamd64.6.2]
;; For 8812A Linksys			================================================================
%Linksys_003F.DeviceDesc%		= RTL8812auBelkin.ndi, USB\VID_13B1&PID_003F

[Amped.NTamd64.6.2]
;; For 8812A Amped			================================================================
%Amped_9097.DeviceDesc%			= RTL8812au.ndi, USB\VID_148F&PID_9097

[ACTIONTEC.NTamd64.6.2]
;; For 8192D ACTIONTEC			================================================================
;%ScreenBeam.DeviceDesc% 		= Actiontec.ndi, USB\VID_1668&PID_8102

[Qihoo.NTamd64.6.2]

;;----------------------------------------------------------------------------
;; Realtek default installation
;;----------------------------------------------------------------------------



[RTL8192cu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192cu.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; 8188RU 8192cu installation
;;----------------------------------------------------------------------------



[RTL8192cu8188RU.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg, BeautifySignal.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu8188RU.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu8188RU.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192cu8188RU.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; Realtek G mode sku installation
;;----------------------------------------------------------------------------



[RTL8192cu_G.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, Ndis6UsbRxAgg.reg, TxByTimerOnn.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, 11gWirelessMode.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu_G.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192cu_G.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192cu_G.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; Realtek N mode wake on wlan sku installation
;;----------------------------------------------------------------------------



[RTL8192cu_wow.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, Ndis6UsbRxAgg.reg, TxByTimerOnn.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, 11nWirelessMode.reg, CIHVS.reg, WowlanAllEnableNoLPS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192cu_wow.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192cu_wow.ndi.NT.HW]
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.PnPFilterRegistration

[RTL8192cu_wow.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------

;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------



[Belkin.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, Ndis6UsbRxAgg.reg, TxByTimerOnn.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, Belkin.reg, BandWidthSetting.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          	; NdisPhysicalMediumNative802_11

[Belkin.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[Belkin.ndi.NT.HW]
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.PnPFilterRegistration

[Belkin.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8192DU default installation
;;----------------------------------------------------------------------------



[RTL8192du.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, EDCCASupport.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

[RTL8192du0.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du0.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du0.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du0.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

[RTL8192du1.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, ConcurrentMode.reg, 2G40MHzAnd5G40MHz.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du1.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du1.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du1.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------



[BelkinN600.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg,BelkinCustomId.reg,Belkin.reg,BandSet.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN600.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[BelkinN600.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[BelkinN600.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[BelkinN450.ndi.NT]
AddReg				= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G20MHzAnd5G40MHz.reg, BelkinCustomId.reg,Belkin.reg,BandSet.reg, WifiConfig.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN450.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[BelkinN450.ndi.NT.HW]
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.PnPFilterRegistration

[BelkinN450.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[BelkinN300.ndi.NT]
AddReg				= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G20MHzAnd5G20MHz.reg, BelkinCustomId.reg,Belkin.reg,BandSet.reg, WifiConfig.reg
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[BelkinN300.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[BelkinN300.ndi.NT.HW]
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.PnPFilterRegistration

[BelkinN300.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------



[RTL8192du_5G.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg,BandOnly5G.reg, ScanType.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192du_5G.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[RTL8192du_5G.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192du_5G.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------

[ACTIONTEC.ndi.NT]
AddReg			= NDIS_62.reg, RTL8192du.common.reg, Ndis6UsbRxAgg.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, 2G40MHzAnd5G40MHz.reg, EDCCASupport.reg, Actiontec.reg, WifiConfig.reg
Characteristics	= 0x84
BusType			= 15 
CopyFiles		= RTWlanU.CopyFiles
*IfType			= 71            ; IF_TYPE_IEEE80211
*MediaType		= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[ACTIONTEC.ndi.NT.Services]
AddService		= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include = netvwifibus.inf
Needs = VWiFiBus.Services

[ACTIONTEC.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[ACTIONTEC.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8723au default installation
;;----------------------------------------------------------------------------

             

[RTL8723au.ndi.NT]
AddReg				= NDIS_62.reg, RTL8723au.common.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, TimerGPIOSetting8723A.reg, WifiConfig.reg, PnpPreTransOn.reg , WowlanEnableNoLPSNoPatternMatch.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8723au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; Realtek 8723bu default installation
;;----------------------------------------------------------------------------

             

[RTL8723bu.ndi.NT]
AddReg				= NDIS_62.reg, RTL8723au.common.reg, Ndis6UsbRxAgg_Jaguar.reg, ConnectedStandbyEnable.reg, RtlSsOnn.reg, RTLWLAN.reg, Ndis6Set.reg, CIHVS.reg, BandWidthSetting.reg, NdisSS.reg, TimerGPIOSetting8723A.reg, WifiConfig.reg, PnpPreTransOn.reg, LPSOn.reg, IPSOn.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8723bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8723bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8723bu.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; Realtek 8188eu default installation
;;----------------------------------------------------------------------------



[RTL8188eu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg.reg, RtlSsOnn.reg, 11nWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8188eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8188eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8188eu.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; Realtek 8811AU default installation
;;----------------------------------------------------------------------------



[RTL8811au.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8811au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8821auLC.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg, WowlanEnableNoLPSNoPatternMatch.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821auLC.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821auLC.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8821auLC.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles





[RTL8811au_PCI.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 5G11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au_PCI.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au_PCI.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8811au_PCI.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles





[RTL8811au_IO_DATA.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, 5G11acWirelessMode.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOff.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8811AU_COMMON.reg, TcpReorderEnable.reg, ScanType.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8811au_IO_DATA.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8811au_IO_DATA.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8811au_IO_DATA.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8812AU default installation
;;----------------------------------------------------------------------------



[RTL8812au.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg, VHT24G.reg,HAdhoc.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812au_Vx.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, USBModeVx.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71         ; IF_TYPE_IEEE80211
*MediaType			= 16         ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812au_Vx.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812au_Vx.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812au_Vx.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812auBelkin.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_Belkin.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auBelkin.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auBelkin.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812auBelkin.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812autplink.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, USBSwitch3.reg, WifiConfig.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812autplink.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812autplink.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812autplink.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles





[RTL8812auDLink.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_DLink.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auDLink.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auDLink.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812auDLink.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;; NEC 8812AU default installation
;;----------------------------------------------------------------------------



[RTL8812auNEC.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, CustomerID_NEC.reg, NEC.reg, Signal.reg, sifs.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auNEC.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auNEC.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812auNEC.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles




[RTL8812auASUS.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTL8812au.common.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomerID_ASUS.reg, CustomTxPwrConfigFile.reg, LDPC_CONFIG.reg, STBC_CONFIG.reg, BEAM_CONFIG.reg, USBSwitch.reg, ScanType.reg, WifiConfig.reg,VHT24G.reg,HAdhoc.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8812auASUS.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8812auASUS.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8812auASUS.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles

;;----------------------------------------------------------------------------
;;----------------------------------------------------------------------------



[RTL8192eu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, Ndis6UsbRxAgg_Jaguar.reg, 11nWirelessMode.reg, RtlSsOff.reg,TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSettingCommon.reg, RTL8192EU_COMMON.reg, TcpReorderEnable.reg, WifiConfig.reg
Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8192eu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8192eu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8192eu.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8814AU default installation
;;----------------------------------------------------------------------------



[RTL8814au.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, WifiConfig.reg, RTL8814au.common.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8814au.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8814au.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8814au.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;----------------------------------------------------------------------------
;; Realtek 8821BU default installation
;;----------------------------------------------------------------------------



[RTL8821bu.ndi.NT]
AddReg				= NDIS_62.reg, UsbCommon.reg, RTLWLAN.reg, RtlSsOnn.reg, 11acWirelessMode.reg, TxByTimerOnn.reg, Ndis6Set.reg, CIHVS.reg, TimerGPIOSetting8812AU.reg, TcpReorderEnable.reg, EarlyModeDisable.reg, CustomTxPwrConfigFile.reg, WifiConfig.reg, RTL8814au.common.reg

Include         	= netvwifibus.inf
Needs				= VWiFiBus.CopyFiles
Characteristics		= 0x84
BusType				= 15 
CopyFiles			= RTWlanU.CopyFiles
*IfType				= 71            ; IF_TYPE_IEEE80211
*MediaType			= 16            ; NdisMediumNative802_11
*PhysicalMediaType	= 9          ; NdisPhysicalMediumNative802_11

[RTL8821bu.ndi.NT.Services]
AddService			= RtlWlanu, 2, RtlWlanu.Service, RtlWlanu.EventLog
Include 			= netvwifibus.inf
Needs 				= VWiFiBus.Services

[RTL8821bu.ndi.NT.HW]
Include = netvwifibus.inf
Needs 	= VWiFiBus.PnPFilterRegistration

[RTL8821bu.ndi.NT.CoInstallers]
AddReg          = CoInstaller.AddReg
CopyFiles       = CoInstaller.CopyFiles


;;
;; OS relative registry.
;;
[NDIS_62.reg]
HKR, Ndi\Interfaces,	UpperRange, 0, "ndis5,mdcwifi"
HKR, Ndi\Interfaces,	LowerRange, 0, "wlan, ethernet, vwifi"
HKR, Ndi,				Service,    0, "RtlWlanu"
;;
;; OS relative service.
;;
[RtlWlanu.Service]
DisplayName    	= %RtlWlanu.DeviceDesc.DispName%
ServiceType    	= 1		; %SERVICE_KERNEL_DRIVER%
StartType      	= 3		; %SERRVICE_DEMAND_START%
ErrorControl   	= 1		; %SERRVICE_ERROR_NORMAL%
ServiceBinary  	= %12%\rtwlanu.sys
LoadOrderGroup 	= NDIS

;;
;; OS relative event log.
;;
[RtlWlanu.EventLog]
AddReg 			= RtlWlanu.AddEventLog.reg

[RtlWlanu.AddEventLog.reg]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll"
HKR, , TypesSupported  , 0x00010001, 7

;*******************************************************************************
; USB common paramters
;*******************************************************************************
[UsbCommon.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"0"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;; For Different selective suspend power save level. Now support 1 and 2. 2 is better.
HKR,,SSPwrLvl,0,"2"


;; For Different AC mode Rx parameters.
HKR,,AcUsbDmaTime,0,"10"
HKR,,AcUsbDmaSize,0,"5"
HKR,,AcUsbDmaTime2,0,"32"
HKR,,AcUsbDmaSize2,0,"5"


;; For Init mode
HKR,,FWOffload,0,"2"


;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation OS Relative
;-------------------------------------------------------------------------------

[Ndis6UsbRxAgg.reg]
HKR,defaults,UsbRxAggMode,0,"2"
HKR,,UsbRxAggMode,0,"2"
HKR,defaults,UsbRxAggPageCount,0,"16"
HKR,,UsbRxAggPageCount,0,"16"


[Ndis6UsbRxAgg_Jaguar.reg]
HKR,defaults,UsbRxAggMode,0,"1"
HKR,,UsbRxAggMode,0,"1"
HKR,defaults,UsbRxAggPageCount,0,"5"
HKR,,UsbRxAggPageCount,0,"5"
HKR,defaults,UsbRxAggPageTimeout,0,"32"
HKR,,UsbRxAggPageTimeout,0,"32"


;;----------------------------------------------------------------------------
;; Wake on Wlan mode option parameters
;;----------------------------------------------------------------------------
[WowlanEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanDisable.reg]
HKR,,WoWLANLPSLevel,0,"0"

[WowlanAllEnableNoLPS.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[WowlanEnableNoLPSNoPatternMatch.reg]
HKR,,WoWLANLPSLevel,0,"0"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "1"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "0"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

[ConnectedStandbyEnable.reg]
HKR,,WoWLANLPSLevel,0,"2"
HKR,,ARPOffloadEnable,0,"1"
HKR,,GTKOffloadEnable,0,"1"
HKR,,D2ListenIntvl,0,"4"
HKR,,NSOffloadEnable,0,"1"
HKR,,NLOEnable,0,"1"

HKR, Ndi\params\*WakeOnMagicPacket,         ParamDesc,  0, %WakeOnMagicPacket%
HKR, Ndi\params\*WakeOnMagicPacket,         default,    0, "0"
HKR, Ndi\params\*WakeOnMagicPacket,         type,       0, "enum"
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnMagicPacket\enum,    "1",        0, %ENABLE_STR%

HKR, Ndi\params\*WakeOnPattern ,            ParamDesc,  0, %WakeOnPattern%
HKR, Ndi\params\*WakeOnPattern,             default,    0, "1"
HKR, Ndi\params\*WakeOnPattern,             type,       0, "enum"
HKR, Ndi\params\*WakeOnPattern\enum,        "0",        0, %DISABLE_STR%
HKR, Ndi\params\*WakeOnPattern\enum,        "1",        0, %ENABLE_STR%

;; Packet coalescing should be enabled in WHCK test
HKR,defaults,*PacketCoalescing,0,"0"
HKR,,*PacketCoalescing,0,"0"

;-------------------------------------------------------------------------------
;	USB selective suspend.
;-------------------------------------------------------------------------------
[RtlSsOnn.reg]
HKR,,EnableUsbSS,0,"1"
[RtlSsOff.reg]
HKR,,EnableUsbSS,0,"0"

;-------------------------------------------------------------------------------
;	PnP pre-transition handling
;-------------------------------------------------------------------------------
[PnpPreTransOn.reg]
HKR,,PreTransPnP,0,"1"
[PnpPreTransOff.reg]
HKR,,PreTransPnP,0,"0"

;-------------------------------------------------------------------------------
;	TX path selection.
;-------------------------------------------------------------------------------
[TxByTimerOnn.reg]
HKR,,SendPacketByTimer,0,"1"
[TxByTimerOff.reg]
HKR,,SendPacketByTimer,0,"0"

;-------------------------------------------------------------------------------
;	IPS selection.
;-------------------------------------------------------------------------------
[IPSOn.reg]
HKR,defaults,InactivePs,0,"2"
HKR,,InactivePs,0,"2"
[IPSOff.reg]
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

;-------------------------------------------------------------------------------
;	LPS selection.
;-------------------------------------------------------------------------------
[LPSOn.reg]
HKR,defaults,bLeisurePs,0,"1"
HKR,,bLeisurePs,0,"1"
[LPSOff.reg]
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;-------------------------------------------------------------------------------
;     Timer GPIO.
;-------------------------------------------------------------------------------
[TimerGPIOSettingCommon.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"2000"
HKR,,GPIOBack,0,"2000"

[TimerGPIOSetting8723A.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"0"
HKR,,GPIODelay,0,"1000"
HKR,,GPIOBack,0,"1000"

[TimerGPIOSetting8812AU.reg]
;; For GPIO detect setting.
HKR,,TimerGPIO,0,"1"
HKR,,GPIODelay,0,"500"
HKR,,GPIOBack,0,"250"

;---------------------------------------------------------------------------------
;    Customer ID
;---------------------------------------------------------------------------------
[CustomerID_Belkin.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"22"

[CustomerID_DLink.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"44"

[CustomerID_NEC.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"45"

[CustomerID_ASUS.reg]
; For Customer ID setting.
HKR,,CustomerID, 0,"35"

;;----------------------------------------------------------------------------
;; TCP Reorder Control Parameters
;;----------------------------------------------------------------------------
[TcpReorderEnable.reg]
HKR,,TcpReorder,0,"1"
[TcpReorderDisable.reg]
HKR,,TcpReorder,0,"0"

;;----------------------------------------------------------------------------
;; Earlymode Control Parameters
;;----------------------------------------------------------------------------
[EarlyModeEnable.reg]
HKR,,bEarlymodeEnable,0,"1"
[EarlyModeDisable.reg]
HKR,,bEarlymodeEnable,0,"0"

;-------------------------------------------------------------------------------
;	Custom Tx Power Limit And Power By Rate Parameters
;-------------------------------------------------------------------------------
[CustomTxPwrConfigFile.reg]
HKR,,PwrByRateFile,0,""
HKR,,PwrLimitFile,0,""

;-------------------------------------------------------------------------------
; Intel Soft AP Mode Reg
;-------------------------------------------------------------------------------
[Intel.reg]
HKR,Ndi\params\ForcedBstDataRate,        ParamDesc,  0, "Broadcast/Multicast Data Rate"
HKR,Ndi\params\ForcedBstDataRate,        type,       0, "enum"
HKR,Ndi\params\ForcedBstDataRate,        default,    0, "0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "0",        0, "Auto"
HKR,Ndi\params\ForcedBstDataRate\enum,   "2",        0, "1Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "4",        0, "2Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "11",      0, "5.5Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "22",     0, "11Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "12",      0, "6Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "18",     0, "9Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "24",     0, "12Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "36",     0, "18Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "48",     0, "24Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "72",     0, "36Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "96",     0, "48Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "108",     0, "54Mbps"
HKR,Ndi\params\ForcedBstDataRate\enum,   "128",     0, "MCS0"
HKR,Ndi\params\ForcedBstDataRate\enum,   "129",     0, "MCS1"
HKR,Ndi\params\ForcedBstDataRate\enum,   "130",     0, "MCS2"
HKR,Ndi\params\ForcedBstDataRate\enum,   "131",     0, "MCS3"
HKR,Ndi\params\ForcedBstDataRate\enum,   "132",     0, "MCS4"
HKR,Ndi\params\ForcedBstDataRate\enum,   "133",     0, "MCS5"
HKR,Ndi\params\ForcedBstDataRate\enum,   "134",     0, "MCS6"
HKR,Ndi\params\ForcedBstDataRate\enum,   "135",     0, "MCS7"
HKR,Ndi\params\ForcedBstDataRate\enum,   "136",     0, "MCS8"
HKR,Ndi\params\ForcedBstDataRate\enum,   "137",     0, "MCS9"
HKR,Ndi\params\ForcedBstDataRate\enum,   "138",     0, "MCS10"
HKR,Ndi\params\ForcedBstDataRate\enum,   "139",     0, "MCS11"
HKR,Ndi\params\ForcedBstDataRate\enum,   "140",     0, "MCS12"
HKR,Ndi\params\ForcedBstDataRate\enum,   "141",     0, "MCS13"
HKR,Ndi\params\ForcedBstDataRate\enum,   "142",     0, "MCS14"
HKR,Ndi\params\ForcedBstDataRate\enum,   "143",     0, "MCS15"

;*******************************************************************************
; RTL8192du common paramters
;*******************************************************************************
[RTL8192du.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

;; For Earlymode 1:Enable 0:Disable
HKR,,bEarlymodeEnable,,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

HKR,defaults,SupportTxPacketBufferColease,0,"0"
HKR,,SupportTxPacketBufferColease,0,"0"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"18"
HKR,,UsbRxAggBlockCount,0,"18"

HKR,defaults,UsbRxAggBlockTimeout,0,"7"
HKR,,UsbRxAggBlockTimeout,0,"7"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"4"
HKR,,UsbTxAggDescNum,0,"4"


;*******************************************************************************
; RTL8723au common paramters
;*******************************************************************************
[RTL8723au.common.reg]
HKR,defaults,LedCtrl,0,"1"
HKR,,LedCtrl,0,"1"

HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"

HKR,defaults,CcxRm,0,"1"
HKR,,CcxRm,0,"1"

HKR,defaults,CcxOffLineDurUpLimit,0,"0"
HKR,,CcxOffLineDurUpLimit,0,"0"

;; For PDN mode switch.
HKR,,PDNMode,0,"1"

;; For PDN mode switch.
HKR,,DongleSS,0,"1"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation
;-------------------------------------------------------------------------------
HKR,defaults,UsbRxAggBlockCount,0,"8"
HKR,,UsbRxAggBlockCount,0,"8"

HKR,defaults,UsbRxAggBlockTimeout,0,"6"
HKR,,UsbRxAggBlockTimeout,0,"6"

HKR,defaults,UsbRxAggPageTimeout,0,"6"
HKR,,UsbRxAggPageTimeout,0,"6"

HKR,defaults,UsbTxAggMode,0,"1"
HKR,,UsbTxAggMode,0,"1"

HKR,defaults,UsbTxAggDescNum,0,"6"
HKR,,UsbTxAggDescNum,0,"6"

;*******************************************************************************
; RTL8188eu common paramters
;*******************************************************************************
[RTL8188eu.common.reg]
;; For SoftApBss creator side judgement.
HKR,defaults,SoftApBss,0,"5"
HKR,,SoftApBss,0,"5"

;*******************************************************************************
; RTL8812au common paramters
;*******************************************************************************
[RTL8812au.common.reg]

;; For IQK Offload to FW.
HKR,,IQKFWOffload,0,"1"

HKR,defaults,UsbTxAggMode,0,"0"
HKR,,UsbTxAggMode,0,"0"
HKR,,*UsbTxAggMode, 0x00000020, "0"

;*******************************************************************************
; RTL8814au common paramters
;*******************************************************************************
[RTL8814au.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"1"
HKR,,StbcCap,0,"0"
HKR,,LdpcCap,0,"0"
HKR,,BeamformCap,0,"0"

;*******************************************************************************
; RTL8821bu common paramters
;*******************************************************************************
[RTL8821bu.common.reg]
HKR,,UsbRxAggMode,0,"3"
HKR,,IQKFWOffload,0,"1"
HKR,,StbcCap,0,"0"
HKR,,LdpcCap,0,"0"
HKR,,BeamformCap,0,"0"

;;----------------------------------------------------------------------------
;; LDPC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[LDPC_CONFIG.reg]
HKR,Ndi\params\LdpcCap,        ParamDesc,  0, "LdpcCap"
HKR,Ndi\params\LdpcCap,        type,       0, "enum"
HKR,Ndi\params\LdpcCap,        default,    0, "51"
HKR,Ndi\params\LdpcCap\enum,   "0",        0, "LDPC Disable"
HKR,Ndi\params\LdpcCap\enum,   "3",        0, "VHT LDPC TX|RX"
HKR,Ndi\params\LdpcCap\enum,   "1",        0, "VHT LDPC RX"
HKR,Ndi\params\LdpcCap\enum,   "2",        0, "VHT LDPC TX"
HKR,Ndi\params\LdpcCap\enum,   "51",       0, "VHT LDPC TX|RX & HT LDPC TX|RX"
HKR,defaults,LdpcCap,0,"51"
HKR,,LdpcCap,0,"51"
HKR,,LdpcCap,,"51"

;;----------------------------------------------------------------------------
;; STBC config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[STBC_CONFIG.reg]
HKR,Ndi\params\StbcCap,        ParamDesc,  0, "StbcCap"
HKR,Ndi\params\StbcCap,        type,       0, "enum"
HKR,Ndi\params\StbcCap,        default,    0, "51"
HKR,Ndi\params\StbcCap\enum,   "0",        0, "STBC Disable"
HKR,Ndi\params\StbcCap\enum,   "3",        0, "VHT STBC TX|RX"
HKR,Ndi\params\StbcCap\enum,   "1",        0, "VHT STBC RX"
HKR,Ndi\params\StbcCap\enum,   "2",        0, "VHT STBC TX"
HKR,Ndi\params\StbcCap\enum,   "51",       0, "VHT STBC TX|RX & HT STBC TX|RX"
HKR,defaults,StbcCap,0,"51"
HKR,,StbcCap,0,"51"
HKR,,StbcCap,,"51"

;;----------------------------------------------------------------------------
;; Beamformer config parameters 8812/8814 only now! Other IC need to assign another value.
;;----------------------------------------------------------------------------

[BEAM_CONFIG.reg]
HKR,Ndi\params\BeamformCap,        ParamDesc,  0, "BeamCap"
HKR,Ndi\params\BeamformCap,        type,       0, "enum"
HKR,Ndi\params\BeamformCap,        default,    0, "51"
HKR,Ndi\params\BeamformCap\enum,   "0",        0, "BEAM Disable"
HKR,Ndi\params\BeamformCap\enum,   "3",        0, "VHT BEAM TX|RX"
HKR,Ndi\params\BeamformCap\enum,   "1",        0, "VHT BEAM TX"
HKR,Ndi\params\BeamformCap\enum,   "2",        0, "VHT BEAM RX"
HKR,Ndi\params\BeamformCap\enum,   "51",       0, "VHT BEAM TX|RX & HT BEAM TX|RX"
HKR,defaults,BeamformCap,0,"34"
HKR,,BeamformCap,0,"34"
HKR,,BeamformCap,,"34"

;;----------------------------------------------------------------------------
;; Realtek WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTLWLAN.reg]
HKR,defaults,Channel,0,"1"
HKR,,Channel,0,"1"

HKR,defaults,StaUapsd,0,"0"
HKR,,StaUapsd,0,"0"

;;Tx power limit
HKR,,EnableTxPowerLimit,0,"2"

;; For QoS test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\QoS,        ParamDesc,  0, "QoS Support"
HKR,Ndi\params\QoS,        type,       0, "enum"
HKR,Ndi\params\QoS,        default,    0, "0"
HKR,Ndi\params\QoS\enum,   "0",        0, "Not Support QoS"
HKR,Ndi\params\QoS\enum,   "1",        0, "Support QoS"
HKR,Ndi\params\QoS\enum,   "2",        0, "Auto"
HKR,defaults,QoS,0,"1"
HKR,,QoS,0,"1"
HKR,,QoS,,"1"


HKR,defaults,RxReorder,0,"1"
HKR,,RxReorder,0,"1"

HKR,,DefaultKeyID,,"0"
HKR,,DefaultKey0,,""
HKR,,DefaultKey1,,""
HKR,,DefaultKey2,,""
HKR,,DefaultKey3,,""

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

HKR,,WEPinNmode,0,"0"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

;-------------------------------------------------------------------------------
;	Some function ability setting
;-------------------------------------------------------------------------------
HKR,defaults,UPDMEnable,0,"1"
HKR,,UPDMEnable,0,"1"

HKR,defaults,LinkSpeedLevel,0,"0"
HKR,,LinkSpeedLevel,0,"0"

HKR,defaults,AutoConnect,0,"1"
HKR,,AutoConnect,0,"1"

HKR,defaults,RWRetry,0,"0"
HKR,,RWRetry,0,"0"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,TxMode,0,"0"
HKR,,TxMode,0,"0"

HKR,defaults,PwrTblSel,0,"0"
HKR,,PwrTblSel,0,"0"
HKR,defaults,PwrByRate,0,"0"
HKR,,PwrByRate,0,"0"
HKR,defaults,PwrRaTbl1,0,"0"
HKR,,PwrRaTbl1,0,"0"
HKR,defaults,PwrRaTbl2,0,"0"
HKR,,PwrRaTbl2,0,"0"
HKR,defaults,PwrRaTbl3,0,"0"
HKR,,PwrRaTbl3,0,"0"
HKR,defaults,PwrRaTbl4,0,"0"
HKR,,PwrRaTbl4,0,"0"
HKR,defaults,PwrRaTbl5,0,"0"
HKR,,PwrRaTbl5,0,"0"
HKR,defaults,PwrRaTbl6,0,"0"
HKR,,PwrRaTbl6,0,"0"
HKR,defaults,PwrRaTbl7,0,"0"
HKR,,PwrRaTbl7,0,"0"
HKR,defaults,PwrRaTbl8,0,"0"
HKR,,PwrRaTbl8,0,"0"
HKR,defaults,PwrRaTbl9,0,"0"
HKR,,PwrRaTbl9,0,"0"
HKR,defaults,PwrRaTbl10,0,"0"
HKR,,PwrRaTbl10,0,"0"
HKR,defaults,PwrRaTbl11,0,"0"
HKR,,PwrRaTbl11,0,"0"
HKR,defaults,PwrRaTbl12,0,"0"
HKR,,PwrRaTbl12,0,"0"
HKR,defaults,PwrRaTbl13,0,"0"
HKR,,PwrRaTbl13,0,"0"
HKR,defaults,PwrRaTbl14,0,"0"
HKR,,PwrRaTbl14,0,"0"
HKR,defaults,PwrRaTbl15,0,"0"
HKR,,PwrRaTbl15,0,"0"
HKR,defaults,PwrRaTbl16,0,"0"
HKR,,PwrRaTbl16,0,"0"

HKR,defaults,GainOffsetFCCLow,0,"0"
HKR,,GainOffsetFCCLow,0,"0"
HKR,defaults,GainOffsetFCC,0,"0"
HKR,,GainOffsetFCC,0,"0"
HKR,defaults,GainOffsetFCCHigh,0,"0"
HKR,,GainOffsetFCCHigh,0,"0"

HKR,defaults,GainOffsetMKKLow,0,"0"
HKR,,GainOffsetMKKLow,0,"0"
HKR,defaults,GainOffsetMKK,0,"0"
HKR,,GainOffsetMKK,0,"0"
HKR,defaults,GainOffsetMKKHigh,0,"0"
HKR,,GainOffsetMKKHigh,0,"0"

HKR,defaults,GainOffsetETSILow,0,"0"
HKR,,GainOffsetETSILow,0,"0"
HKR,defaults,GainOffsetETSI,0,"0"
HKR,,GainOffsetETSI,0,"0"
HKR,defaults,GainOffsetETSIHigh,0,"0"
HKR,,GainOffsetETSIHigh,0,"0"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

;Dynamic batch indication
HKR,defaults,DynamicBatchEnable,0,"1"
HKR,,DynamicBatchEnable,0,"1"

HKR,defaults,BINumber,0,"10"
HKR,,BINumber,0,"10"

HKR,Ndi\params\EnableAdaptivity, 		ParamDesc, 	0, "EnableAdaptivity"
HKR,Ndi\params\EnableAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\EnableAdaptivity, 		default, 	0, "2"
HKR,Ndi\params\EnableAdaptivity\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"1", 		0, "Enable"
HKR,Ndi\params\EnableAdaptivity\enum, 	"2", 		0, "Auto"
HKR,defaults,EnableAdaptivity, 0, "2"
HKR,,EnableAdaptivity, 0, "2"

HKR,Ndi\params\L2HForAdaptivity, 		ParamDesc, 	0, "L2HForAdaptivity"
HKR,Ndi\params\L2HForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\L2HForAdaptivity, 		default, 	0, "F5"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"245", 		0, "F5"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"243", 		0, "F3"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"241", 		0, "F1"
HKR,Ndi\params\L2HForAdaptivity\enum, 	"239", 		0, "EF"
HKR,defaults,L2HForAdaptivity, 0, "245"
HKR,,L2HForAdaptivity, 0, "245"

HKR,Ndi\params\HLDiffForAdaptivity, 		ParamDesc, 	0, "HLDiffForAdaptivity"
HKR,Ndi\params\HLDiffForAdaptivity, 		type, 		0, "enum"
HKR,Ndi\params\HLDiffForAdaptivity, 		default, 	0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"7", 		0, "7"
HKR,Ndi\params\HLDiffForAdaptivity\enum, 	"9", 		0, "9"
HKR,defaults,HLDiffForAdaptivity, 0, "7"
HKR,,HLDiffForAdaptivity, 0, "7"

[Ndis5Set.reg]
HKR,Ndi\params\PSPXlinkMode,			ParamDesc,  0, %PSP_XLINK_STR%
HKR,Ndi\params\PSPXlinkMode,			type,       0, "enum"
HKR,Ndi\params\PSPXlinkMode,			default,    0, "0"
HKR,Ndi\params\PSPXlinkMode\enum,		"0",        0, %DISABLE_STR%
HKR,Ndi\params\PSPXlinkMode\enum,		"1",        0, %ENABLE_STR%
HKR,defaults,PSPXlinkMode,0,"0"
HKR,,PSPXlinkMode,0,"0"

; Hw Beacon Max Error
HKR,,bBcnMaxErrorRegEnable,0,"0"

;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"0"
HKR,,AggDMEnable,0,"0"

[Ndis6Set.reg]
;Inactive Power Save
HKR,defaults,InactivePs,0,"0"
HKR,,InactivePs,0,"0"

HKR,defaults,AggDMEnable,0,"1"
HKR,,AggDMEnable,0,"1"

[NEC.reg]
HKR,Ndi\params\TxPwrPercentage, 	ParamDesc, 	0, %TX_PWR_CONTROL_STR%
HKR,Ndi\params\TxPwrPercentage, 	type, 		0, "enum"
HKR,Ndi\params\TxPwrPercentage, 	default, 	0, "8"
HKR,Ndi\params\TxPwrPercentage\enum, 	"1", 		0, %TX_PWR_PERCENTAGE_1_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"2", 		0, %TX_PWR_PERCENTAGE_2_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"4", 		0, %TX_PWR_PERCENTAGE_3_STR%
HKR,Ndi\params\TxPwrPercentage\enum, 	"8", 		0, %TX_PWR_PERCENTAGE_4_STR%
HKR,defaults,TxPwrPercentage, 0, "8"
HKR,,TxPwrPercentage, 0, "8"

HKR,Ndi\params\StreamMode, 	ParamDesc, 	0, %STREAM_MODE_STR%
HKR,Ndi\params\StreamMode, 	type, 		0, "enum"
HKR,Ndi\params\StreamMode, 	default, 	0, "0"
HKR,Ndi\params\StreamMode\enum, 	"0", 		0, "OFF"
HKR,Ndi\params\StreamMode\enum, 	"1", 		0, "ON"
HKR,defaults,StreamMode, 0, "0"
HKR,,StreamMode, 0, "0"

;Leisure Power Save
HKR,defaults,bLeisurePs,0,"0"
HKR,,bLeisurePs,0,"0"

;Fw Control LPS
HKR,defaults,bFwCtrlLPS,0,"1"
HKR,,bFwCtrlLPS,0,"1"

;; LPS Interval
;HKR,defaults,LPSIntvl,0,"5"
HKR,,LPSIntvl,0,"5"

;BTmode
HKR,,bBTMode,0,"1"

; Reset Tx Hang
HKR,defaults,USBResetTxHang,0,"1"
HKR,,USBResetTxHang,0,"1"

; OS protocol offload detection and decision
HKR,,ProtocolOffloadDecision,0,"1"

; Win8 FSS mode detection mechanism
HKR,,FSSDetection,0,"1"

HKR,defaults,MultiMode,0,"1"
HKR,,MultiMode,0,"1"

HKR,defaults,RxSC,0,"0"
HKR,,RxSC,0,"0"

HKR,defaults,TxSC,0,"0"
HKR,,TxSC,0,"0"

; /****************************************************************************
; ** Customerize Registry Area.
; ****************************************************************************/
[USBSwitch.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "0"
HKR,,ForcedUsbMode, 0, "0"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"10"
HKR,,UsbSwitchSpeed,0,"10"

HKR,defaults,UsbSwitchThL,0,"35"
HKR,,UsbSwitchThL,0,"35"

HKR,defaults,UsbSwitchThH,0,"45"
HKR,,UsbSwitchThH,0,"45"

HKR,defaults,UsbSwitchThRssi,0,"40"
HKR,,UsbSwitchThRssi,0,"40"

HKR,defaults,ViaU3,0,"0"
HKR,,ViaU3,0,"0"


HKR,defaults,ChannelPlan, 0, %CHNL_PLAN_VALUE%
HKR,,ChannelPlan, 0, %CHNL_PLAN_VALUE%

[USBSwitch3.reg]
HKR,Ndi\params\ForcedUsbMode, 	ParamDesc, 	0, "USB Switch Mode"
HKR,Ndi\params\ForcedUsbMode, 	type, 		0, "enum"
HKR,Ndi\params\ForcedUsbMode, 	default, 	0, "0"
HKR,Ndi\params\ForcedUsbMode\enum, 	"0", 	0, "Auto"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"1", 	0, "USB 2.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"2", 	0, "USB 3.0"
;;HKR,Ndi\params\ForcedUsbMode\enum, 	"3", 	0, "USB Mode 1"
HKR,Ndi\params\ForcedUsbMode\enum, 	"4", 	0, "USB Mode 2"
HKR,Ndi\params\ForcedUsbMode\enum, 	"8", 	0, "USB Mode 3"
HKR,defaults,ForcedUsbMode, 0, "8"
HKR,,ForcedUsbMode, 0, "8"

HKR,Ndi\params\UsbSwFast, 	ParamDesc, 	0, "USB SF Mode"
HKR,Ndi\params\UsbSwFast, 	type, 		0, "enum"
HKR,Ndi\params\UsbSwFast, 	default, 	0, "0"
HKR,Ndi\params\UsbSwFast\enum, 	"0", 	0, "Disable"
HKR,Ndi\params\UsbSwFast\enum, 	"1", 	0, "Enable"
HKR,defaults,UsbSwFast,0,"0"
HKR,,UsbSwFast,0,"0"

HKR,defaults,UsbSwitchSpeed,0,"50"
HKR,,UsbSwitchSpeed,0,"50"

HKR,defaults,UsbSwitchThL,0,"20"
HKR,,UsbSwitchThL,0,"20"

HKR,defaults,UsbSwitchThH,0,"5"
HKR,,UsbSwitchThH,0,"5"

HKR,defaults,UsbSwitchThRssi,0,"35"
HKR,,UsbSwitchThRssi,0,"35"

HKR,defaults,ViaU3,0,"0"
HKR,,ViaU3,0,"0"


HKR,defaults,ChannelPlan, 0, %CHNL_PLAN_VALUE%
HKR,,ChannelPlan, 0, %CHNL_PLAN_VALUE%

[USBModeVx.reg]
HKR,defaults,ForcedUsbMode, 0, "5"
HKR,,ForcedUsbMode, 0, "5"        

[Signal.reg]
HKR,defaults,LinkSpeedLevel, 0, "28"
HKR,,LinkSpeedLevel, 0, "28"

[BeautifySignal.reg]
HKR,Ndi\params\LinkSpeedLevel, 	ParamDesc, 	0, "Beautify Signal Strength Level"
HKR,Ndi\params\LinkSpeedLevel, 	type, 		0, "enum"
HKR,Ndi\params\LinkSpeedLevel, 	default, 	0, "0"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"0", 	0, "Default"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"52", 	0, "SS Display Lvl1"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"54", 	0, "SS Display Lvl2"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"56", 	0, "SS Display Lvl3"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"58", 	0, "SS Display Lvl4"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"60", 	0, "SS Display Lvl5"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"62", 	0, "SS Display Lvl6"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"64", 	0, "SS Display Lvl7"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"68", 	0, "SS Display Lvl8"
HKR,Ndi\params\LinkSpeedLevel\enum, 	"70", 	0, "SS Display Lvl9"
HKR,defaults,LinkSpeedLevel, 0, "0"
HKR,,LinkSpeedLevel, 0, "0"


[sifs.reg]
HKR,defaults,SifsThresh, 0, "0"
HKR,,SifsThresh, 0, "0"


[ScanType.reg]
HKR,defaults,PassiveScan, 0, "0"
HKR,,PassiveScan, 0, "0"

; /****************************************************************************
; ** IHV Service Reg for CCX
; ****************************************************************************/
[CIHVS.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL,       0,  "%SystemRoot%\system32\Rtlihvs.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID,   0,  "{6C2A8CCA-B2A2-4d81-A3B2-4E15F445C312}"
HKR, Ndi\IHVExtensions, GroupName,              0,  "Realtek CCX SDK IHV Service"
HKR, Ndi\IHVExtensions, AdapterOUI,             0x00010001, 0x00e04c

;;----------------------------------------------------------------------------
;; Belkin WLAN NIC parameters
;;----------------------------------------------------------------------------
[Belkin.reg]
HKR,Ndi\params\RFOff,			ParamDesc,  0, "Radio"
HKR,Ndi\params\RFOff,			type,       0, "enum"
HKR,Ndi\params\RFOff,			default,    0, "0"
HKR,Ndi\params\RFOff\enum,		"0",        0, "On"
HKR,Ndi\params\RFOff\enum,		"1",        0, "Off"
HKR,defaults,RFOff,0,"0"
HKR,,RFOff,0,"0"

;;----------------------------------------------------------------------------
;; Wireless Mode Related Parameters
;;----------------------------------------------------------------------------
[11nWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %IEEE_802_11BGN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,,BWSetting,0,"1"

HKR,,Channel,0,"10"

[11gWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,defaults,WirelessMode, 0, "4"
HKR,,WirelessMode, 0, "4"

HKR,,BWSetting,0,"0"

HKR,,Channel,0,"10"

[11agnWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

[11acWirelessMode.reg]
HKR,Ndi\params\WirelessMode, 		ParamDesc, 	0, %WL_MODE_STR%
HKR,Ndi\params\WirelessMode, 		type, 		0, "enum"
HKR,Ndi\params\WirelessMode, 		default, 	0, "8"
HKR,Ndi\params\WirelessMode\enum, 	"8", 		0, %AUTO_STR%
HKR,Ndi\params\WirelessMode\enum, 	"1", 		0, %IEEE_802_11A_STR%
HKR,Ndi\params\WirelessMode\enum, 	"2", 		0, %IEEE_802_11B_STR%
HKR,Ndi\params\WirelessMode\enum, 	"4", 		0, %IEEE_802_11BG_STR%
HKR,Ndi\params\WirelessMode\enum, 	"16", 		0, %IEEE_802_11BGN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"32", 		0, %IEEE_802_11AN_STR%
HKR,Ndi\params\WirelessMode\enum, 	"64", 		0, %IEEE_802_11ANAC_STR%
HKR,Ndi\params\WirelessMode\enum, 	"256", 		0, %IEEE_802_11AC_STR%
HKR,defaults,WirelessMode, 0, "8"
HKR,,WirelessMode, 0, "8"

HKR,,Channel,0,"10"
HKR,,RFType,0,"15"

HKR,,BWSetting,0,"2"

[5G11acWirelessMode.reg]
HKR,,WirelessMode, 0, "64"
HKR,,Channel,0,"36"
HKR,,RFType,0,"15"
HKR,,BWSetting,0,"2"

;;----------------------------------------------------------------------------
;; 11AC series IC VHT 2.4G Support
;;----------------------------------------------------------------------------
[VHT24G.reg]
HKR,Ndi\params\Vht24g, 		ParamDesc, 	0, "VHT 2.4G"
HKR,Ndi\params\Vht24g, 		type, 		0, "enum"
HKR,Ndi\params\Vht24g, 		default, 	0, "0"
HKR,Ndi\params\Vht24g\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\Vht24g\enum, 	"1", 		0, "Enable"
HKR,defaults,Vht24g, 0, "0"
HKR,,Vht24g, 0, "0"

;;----------------------------------------------------------------------------
;; 11N or higher Adhoc Mode
;;----------------------------------------------------------------------------
[HAdhoc.reg]
HKR,Ndi\params\11nAdhoc, 		ParamDesc, 	0, "High Adhoc Mode"
HKR,Ndi\params\11nAdhoc, 		type, 		0, "enum"
HKR,Ndi\params\11nAdhoc, 		default, 	0, "0"
HKR,Ndi\params\11nAdhoc\enum, 	"0", 		0, "Disable"
HKR,Ndi\params\11nAdhoc\enum, 	"1", 		0, "Enable"
HKR,defaults,11nAdhoc, 0, "0"
HKR,,11nAdhoc, 0, "0"

;;----------------------------------------------------------------------------
;; Usb selective suspend parameters
;;----------------------------------------------------------------------------
[NdisSS.reg]
HKR,Ndi\params\*SelectiveSuspend,	    ParamDesc,  0, %SelectiveSuspend%
HKR,Ndi\params\*SelectiveSuspend,	    default,    0, "1"
HKR,Ndi\params\*SelectiveSuspend,	    type,       0, "enum"
HKR,Ndi\params\*SelectiveSuspend\enum,   "0",        0, "Disabled"
HKR,Ndi\params\*SelectiveSuspend\enum,   "1",        0, "Enabled"

HKR,Ndi\params\*SSIdleTimeout,	    ParamDesc,  0, %SSIdleTimeout%
HKR,Ndi\params\*SSIdleTimeout,	    type,       0, "int"
HKR,Ndi\params\*SSIdleTimeout,	    default,    0, "10"
HKR,Ndi\Params\*SSIdleTimeout,      Max,        0, "60"
HKR,Ndi\Params\*SSIdleTimeout,      Min,        0, "5"
HKR,Ndi\Params\*SSIdleTimeout,      Step,       0, "1"

HKR,,*SSIdleTimeout, 0, "10"


;*******************************************************************************
; Two STA Concurrent Mode Reg
;*******************************************************************************
[ConcurrentMode.reg]
HKR,Ndi\params\TwoStaConcurrentMode,		ParamDesc,  0, %TWO_STA_CONCURRENT_MODE%
HKR,Ndi\params\TwoStaConcurrentMode,		type,       0, "enum"
HKR,Ndi\params\TwoStaConcurrentMode,			default,    0, "1"
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"0",        0, %SECONDARY_DISABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"1",        0, %SECONDARY_ENABLE%
HKR,Ndi\params\TwoStaConcurrentMode\enum,		"2",        0, %SECONDARY_AUTO%
HKR,defaults,TwoStaConcurrentMode,0,"0"
HKR,,TwoStaConcurrentMode,0,"0"

;*******************************************************************************
; bandwidth setting
;*******************************************************************************
[2G40MHzAnd5G40MHz.reg]
HKR,Ndi\params\BW40MHzFor2G,        ParamDesc,  0, "Bandwidth_2.4G"
HKR,Ndi\params\BW40MHzFor2G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor2G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor2G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor2G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,0,"1"
HKR,,BW40MHzFor2G,,"1"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G40MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,Ndi\params\BW40MHzFor5G,        ParamDesc,  0, "Bandwidth_5G"
HKR,Ndi\params\BW40MHzFor5G,        type,       0, "enum"
HKR,Ndi\params\BW40MHzFor5G,        default,    0, "1"
HKR,Ndi\params\BW40MHzFor5G\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BW40MHzFor5G\enum,   "1",        0, "20_40MHz"
HKR,defaults,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,0,"1"
HKR,,BW40MHzFor5G,,"1"

[2G20MHzAnd5G20MHz.reg]
HKR,defaults,BW40MHzFor2G,0,"0"
HKR,,BW40MHzFor2G,0,"0"

HKR,defaults,BW40MHzFor5G,0,"0"
HKR,,BW40MHzFor5G,0,"0"

[BandWidthSetting.reg]
;; 40MHz Support in 11n
HKR,Ndi\params\BWSetting,        ParamDesc,  0, "Bandwidth"
HKR,Ndi\params\BWSetting,        type,       0, "enum"
HKR,Ndi\params\BWSetting,        default,    0, "1"
HKR,Ndi\params\BWSetting\enum,   "0",        0, "20MHz Only"
HKR,Ndi\params\BWSetting\enum,   "1",        0, "20_40MHz"
HKR,defaults,BWSetting,0,"1"
HKR,,BWSetting,0,"1"
HKR,,BWSetting,,"1"

[BelkinCustomId.reg]
HKR,,CustomerID,0,"21"
HKR,,CustomerID,,"21"

[BandSet.reg]
HKR,Ndi\params\WirelessBand,			ParamDesc,  0, "Disable Bands"
HKR,Ndi\params\WirelessBand,			type,       0, "enum"
HKR,Ndi\params\WirelessBand,			default,    0, "0"
HKR,Ndi\params\WirelessBand\enum,		"0",        0, "Disable 11A"
HKR,Ndi\params\WirelessBand\enum,		"1",        0, "Disable 11B/G"
HKR,Ndi\params\WirelessBand\enum,		"2",        0, "None"
HKR,defaults,WirelessBand,0,"2"
HKR,,WirelessBand,0,"2"

[BandOnly5G.reg]
HKR,defaults,WirelessBand,0,"1"
HKR,,WirelessBand,0,"1"

;*****************************************************************************
; 92DU VS open EDCCA 
;*****************************************************************************
[EDCCASupport.reg]
HKR,defaults,EdccaSupport,0,"0"
HKR,,EdccaSupport,0,"0"


;*****************************************************************************
; For Wifi config
;*****************************************************************************
[WifiConfig.reg]
;; For WiFi test, 1: WiFi Config and 0: Performance Config
HKR,Ndi\params\WiFiConfg,        ParamDesc,  0, "WiFi Config"
HKR,Ndi\params\WiFiConfg,        type,       0, "enum"
HKR,Ndi\params\WiFiConfg,        default,    0, "0"
HKR,Ndi\params\WiFiConfg\enum,   "0",        0, "Performance"
HKR,Ndi\params\WiFiConfg\enum,   "1",        0, "WiFi"
HKR,defaults,WiFiConfg,0,"0"
HKR,,WiFiConfg,0,"0"
HKR,,WiFiConfg,,"0"

;;----------------------------------------------------------------------------
;; 8811AU/8821AU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8811AU_COMMON.reg]
HKR,,EnableTxPowerLimit,0,"0"
HKR,,TxDutyEnable,0,"1"
HKR,,StbcCap,0,"17"
HKR,,RxSPStream,0,"1"
HKR,,RspPwr, 0, "1"

HKR,defaults,UsbTxAggDescNum,0,"10"
HKR,,UsbTxAggDescNum,0,"10"

HKR,,DecryptCustomFile,,"1"
HKR,,PwrByRateFile,0,"EncPWT.txt"
HKR,,PwrLimitFile,0,"TXPWR_LMT.txt"

HKR,,LdpcCap,0,"34"

HKR,,HWRTSEnable,,"1"

HKR,,BeamformCap,0,"34"

;;----------------------------------------------------------------------------
;; 8192EU WLAN NIC parameters
;;----------------------------------------------------------------------------
[RTL8192EU_COMMON.reg]
HKR,defaults,UsbTxAggDescNum,0,"15"
HKR,,UsbTxAggDescNum,0,"15"
HKR,,DisableBTCoexist,0,"1"
HKR,,WoWLANMode, 0, "0"

HKR,,LdpcCap,0,"0"
HKR,,StbcCap,0,"48"
HKR,,BeamformCap,0,"48"

HKR,,bEarlymodeEnable,0,"0"

;;----------------------------------------------------------------------------
;; Actiontec WLAN NIC parameters
;;----------------------------------------------------------------------------
[Actiontec.reg]
HKR,defaults,VWifiSupport,0,"0"
HKR,,VWifiSupport,0,"0"

;*******************************************************************************
; WAPI IHV section
;*******************************************************************************
[ihvwapi.reg]
HKR, Ndi\IHVExtensions, ExtensibilityDLL, 0, "%SystemRoot%\system32\ihvwapi.dll"
HKR, Ndi\IHVExtensions, UIExtensibilityCLSID, 0, "{4A01f9f9-6012-4343-A8C4-10B5DF32672A}"
HKR, Ndi\IHVExtensions, GroupName, 0, "Wireless 802.11 IHV WAPI Config UI"
HKR, Ndi\IHVExtensions, AdapterOUI, 0x00010001, 0x00e04c

[RegisterWAPIIHVUIExt]
11,,ihvwapiui.dll,1

;*******************************************************************************
; Destination Directory
;*******************************************************************************
[RTWlanU.CopyFiles]
rtwlanu.sys,,,2

[DestinationDirs]
DefaultDestDir     	= 11
RTWlanU.CopyFiles	= 12
CoInstaller.CopyFiles = 11

;;****************************************************************************
;; Source Files
;;****************************************************************************
[SourceDisksFiles]
rtwlanu.sys = 1
rtlCoInst.dll = 1
rtlCoInst.dat = 1

[SourceDisksNames]
1=%DISKNAME%,,,
[CoInstaller.AddReg]
HKR,,CoInstallers32,0x10000,"rtlCoInst.DLL,rtlCoInst"

[CoInstaller.CopyFiles]
rtlCoInst.dll,,,0x04
rtlCoInst.dat,,,0x04
;*******************************************************************************
; Strings
;*******************************************************************************
[Strings]
SSID_STR					= "SSID"
CHNL_PLAN_VALUE             = 127
CHANNEL_STR					= "Channel"
NETWORK_TYPE_STR			= "Network Type"
LED_CONTROL_STR				= "LED Control" 
POWER_SAVE_STR				= "Power Save Mode"
WIFI_IBSS_STR				= "IBSS Default 11b Mode"
RATE_ADAPTIVE_STR			= "Rate Adaptive"
QOS_STR						= "QoS"
WiFiConfg_STR	  			= "WiFiConfg"
WMM_APSD					= "WMM APSD"
CCX_RM_STR					= "CCX Radio Measurement"
CCX_OFF_LINE_DUR_UP_LIMIT_STR		= "CCX Max Off-Line Measurement (0: unlimited)"
HW_PARA_STR					= "Init from HwParaFile"
THREE_WIRE_MODE_STR			= "Three Wire Programming Mode"
BOARD_TYPE_STR				= "Board Type"
PROTECTION_MODE_STR			= "Protection Mode"
TPC_STR						= "Transmit Power Control"
TPC_POLARITY_STR			= "TPC Polarity Select"
HIGH_POWER_STR				= "High Power Mechanism"
INIT_GAIN_STR				= "Initial Gain State"
CW_MAX_MIN_STR				= "Contention Window"
PSP_XLINK_STR				= "PSP XLink Mode"
DISABLE_STR					= "Disable"
ENABLE_STR					= "Enable"
AD_HOC_STR					= "Ad Hoc"
INFRASTRUCTURE_STR			= "Infrastructure"
AUTO_SELECT					= "Auto select"
WL_MODE_STR					= "Wireless Mode"
RX_REORDER_STR				= "Rx Reorder"
CAM_STR						= "CAM"
MAX_PSP_STR					= "MAX_PSP"
Fast_PSP_STR				= "Fast_PSP"
NO_AC_STR					= "No AC (Disable)"
ALL_AC_STR					= "ALL AC"
AUTO_STR 				= "Auto"
IEEE_802_11A_STR 			= "IEEE 802.11a"
IEEE_802_11B_STR 			= "IEEE 802.11b"
IEEE_802_11BG_STR 			= "IEEE 802.11b/g"
IEEE_802_11BGN_STR 			= "IEEE 802.11b/g/n"
IEEE_802_11AN_STR			= "IEEE 802.11a/n"
IEEE_802_11ANAC_STR			= "IEEE 802.11a/n/ac"
IEEE_802_11AC_STR			= "IEEE 802.11 ac"
SelectiveSuspend               		= "Selective suspend"
SSIdleTimeout                  		= "Selective suspend Timeout"

TX_PWR_CONTROL_STR		= "送信出力"
TX_PWR_PERCENTAGE_1_STR 	= "12.5%"
TX_PWR_PERCENTAGE_2_STR 	= "25%"
TX_PWR_PERCENTAGE_3_STR 	= "50%"
TX_PWR_PERCENTAGE_4_STR 	= "100%"
STREAM_MODE_STR			= "ストリーミングモード"

WakeOnMagicPacket           = "Wake on Magic Packet"
WakeOnPattern               = "Wake on Pattern Match"
PacketCoalescing		= "D0 Packet Coalescing"

;-------------------------------------------------------------------------------
;	USB Tx/Rx aggregation strings
;-------------------------------------------------------------------------------
RX_AGG_MODE_STR				= "Rx Aggregation Mode"
RX_AGG_MODE_BLOCK_STR		= "Rx Agg USB Block Mode"
RX_AGG_MODE_PAGE_STR		= "Rx Agg DMA Page Mode"
RX_AGG_MODE_MIXED_STR		= "Rx Agg USB and Page Mixed Mode"
RX_AGG_USB_BLOCK_STR		= "Rx Agg USB Block Threshold"
RX_AGG_USB_TIMEOUT_STR		= "Rx Agg USB Timeout"
RX_AGG_DMA_PAGE_STR			= "Rx Agg DMA Page Threshold"
RX_AGG_DMA_TIMEOUT_STR		= "Rx Agg DMA Timeout"
TX_AGG_MODE_STR				= "Tx Aggregation Mode"
TX_AGG_DESC_PER_OUT_STR		= "Tx Agg Number of descriptor per bulk out"

;-------------------------------------------------------------------------------
;	Two STA Concurrent Mode
;-------------------------------------------------------------------------------
TWO_STA_CONCURRENT_MODE		= "Two STA Concurrent Mode"
SECONDARY_DISABLE			= "Secondary client Disable"
SECONDARY_ENABLE			= "Secondary Client Enable"
SECONDARY_AUTO				= "Secondary Client Auto Select"


;*******************************************************************************
; manufacture description
;*******************************************************************************
Realtek					= "Realtek Semiconductor Corp."
PCI             		= "PLANEX COMMUNICATIONS INC"
Sitecom         		= "Sitecom Europe B.V."
EDIMAX         			= "EDIMAX"
ELECOM         			= "ELECOM CO.,LTD."
Abocom					= "AboCom System, Inc."
Amigo					= "Amigo Technology Inc"
Hercules				= "Guillemot Corporation S.A"
DLink					= "D-Link Corporation"
Belkin					= "Belkin International, Inc."
Zyxel					= "ZyXEL"
ATKK					= "Allied Telesis K.K."
TRENDnet				= "TRENDnet"
Feixun					= "Shanghai Feixun Communication Co.,Ltd"
NetweeN					= "NetweeN"
XAVI					= "XAVI Technologies Corp."
Netgear					= "NETGEAR Inc."
Oar_Inc					= "Oar Inc."
ASUS					= "ASUSTeK Computer Inc."
HAWKING					= "Hawking Technologies Inc."
Compare					= "Compare Electronics CO.,LTD"
IO_DATA					= "I-O DATA DEVICE, INC"
TPLINK					= "TP-LINK Technologies Co."
Logitec					= "Logitec Japan"
NEC						= "NEC AccessTechnica, Ltd."
ACTIONTEC				= "Actiontec"
WD						= "Western Digital"
EnGenius				= "EnGenius Technologies."
Linksys					= "Linksys LLC"
BUFFALO					="BUFFALO INC."
Amped					= "Amped Wireless"
Qihoo					= "Qihoo 360 Technology Co.,Ltd"

;*******************************************************************************
;	Source disk name
;*******************************************************************************
;DISKNAME							= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
DISKNAME							= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter Driver Disk"
RtlWlanu.DeviceDesc 				= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"
RtlWlanu.DeviceDesc.DispName		= "Realtek Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc 				= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192cu.DeviceDesc.DispName		= "Realtek RTL8192CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc 				= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188cu_G.DeviceDesc.DispName		= "Realtek RTL8188CU Wireless LAN 802.11 USB 2.0 Network Adapter"
RTL8188ce_vau.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ce_vau_G.DeviceDesc 			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8188ce_vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTL8192ce_vau.DeviceDesc 			= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8192ce_vau.DeviceDesc.DispName	= "Realtek RTL8192CE-VAU Wireless LAN 802.11n USB minicard"
RTL8188cu_slim_solo.DeviceDesc				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_solo_lc.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
RTL8188cu_slim_combo.DeviceDesc				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188cu_slim_combo.DeviceDesc.DispName	= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
RTL8188ru.DeviceDesc 				= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188ru.DeviceDesc.DispName		= "Realtek RTL8188RU Wireless LAN 802.11n USB High Power Dongle"
RTL8188cus_vl.DeviceDesc 			= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188cus_vl.DeviceDesc.DispName	= "Realtek RTL8188CUS-VL Wireless LAN 802.11n USB 2.0 Network Adapter"
RTK_AZ88vau.DeviceDesc				= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau.DeviceDesc.DispName		= "Realtek RTL8188CE-VAU Wireless LAN 802.11n USB minicard"
RTK_AZ88vau_G.DeviceDesc			= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88vau_G.DeviceDesc.DispName	= "Realtek RTL8188CE-VAU Wireless LAN 802.11 USB minicard"
RTK_AZ88cus.DeviceDesc				= "Wireless USB Card"
RTK_AZ88cus.DeviceDesc.DispName		= "Wireless USB Card"
RTL8188ctv.DeviceDesc				= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ctv.DeviceDesc.DispName		= "Realtek RTL8188CTV Wireless LAN 802.11n USB 2.0 Network Adapter"
PCI.DeviceDesc 						= "GW-USValue-EZ"
PCI.DeviceDesc.DispName				= "GW-USValue-EZ"
PCI-2.DeviceDesc 					= "GW-USLight"
PCI-2.DeviceDesc.DispName			= "GW-USLight"
PCI_Abocom88cu.DeviceDesc 			= "GW-USNano2"
PCI_Abocom88cu.DeviceDesc.DispName	= "GW-USNano2"
PCI_Abocom92cu.DeviceDesc 			= "GW-USEco300"
PCI_Abocom92cu.DeviceDesc.DispName	= "GW-USEco300"
PCI_Vencer.DeviceDesc 				= "BT-Micro3H2X Wireless LAN"
PCI_Vencer.DeviceDesc.DispName		= "BT-Micro3H2X Wireless LAN"
Sitecom.DeviceDesc 					= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom.DeviceDesc.DispName			= "Sitecom Wireless Ultra Nano USB Adapter 150N X1 WL-365"
Sitecom_UN.DeviceDesc 				= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_UN.DeviceDesc.DispName		= "Wireless Ultra Nano Network Adapter 150N"
Sitecom_HG.DeviceDesc 				= "Wireless High-gain Network adapter 300N WLA-4001"
Sitecom_HG.DeviceDesc.DispName		= "Wireless High-gain Network adapter 300N WLA-4001"
EDIMAX.DeviceDesc 					= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX.DeviceDesc.DispName			= "150Mbps Wireless 802.11b/g/n Nano USB Adapter"
EDIMAX300.DeviceDesc 				= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
EDIMAX300.DeviceDesc.DispName		= "Edimax 300Mbps wireless 802.11b/g/n USB adapter"
Abocom.DeviceDesc 					= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom.DeviceDesc.DispName			= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom92cu.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Amigo.DeviceDesc 					= "Wireless USB Card"
Amigo.DeviceDesc.DispName			= "Wireless USB Card"
Hercules.DeviceDesc 				= "Hercules Wireless N Pico USB "
Hercules.DeviceDesc.DispName		= "Hercules Wireless N Pico USB "
Hercules-E035.DeviceDesc 			= "Hercules Wireless N Mini v2 USB Key"
Hercules-E035.DeviceDesc.DispName	= "Hercules Wireless N Mini v2 USB Key"
DLink-1.DeviceDesc 					= "D-Link DWA-133 Wireless N USB Adapter"
DLink-1.DeviceDesc.DispName			= "D-Link DWA-133 Wireless N USB Adapter"
DLink-2.DeviceDesc 					= "D-Link DWA-135 Wireless N USB Adapter"
DLink-2.DeviceDesc.DispName			= "D-Link DWA-135 Wireless N USB Adapter"
DLink-3.DeviceDesc 					= "D-Link DWA-121 Wireless N USB Adapter"
DLink-3.DeviceDesc.DispName			= "D-Link DWA-121 Wireless N USB Adapter"
DLink-4.DeviceDesc 					= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-4.DeviceDesc.DispName			= "D-Link DWA-130 Wireless N USB Adapter(rev.F1)"
DLink-5.DeviceDesc 					= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
DLink-5.DeviceDesc.DispName			= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.C)"
Belkin.DeviceDesc 					= "Surf Wireless Micro USB Adapter"
Belkin.DeviceDesc.DispName			= "Surf Wireless Micro USB Adapter"
Belkin-2.DeviceDesc 				= "Belkin Surf & Share Wireless USB Adapter"
Belkin-2.DeviceDesc.DispName		= "Belkin Surf & Share Wireless USB Adapter"
Belkin-3.DeviceDesc 				= "N300 USB Network Adapter"
Belkin-3.DeviceDesc.DispName		= "N300 USB Network Adapter"
Belkin-4.DeviceDesc 				= "Belkin Wireless Adapter"
Belkin-4.DeviceDesc.DispName		= "Belkin Wireless Adapter"
ZyXEL.DeviceDesc 					= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ZyXEL.DeviceDesc.DispName			= "ZyXEL Wireless LAN 802.11n USB 2.0 Network Adapter"
ATKK.DeviceDesc						= "Corega CG-WLUSB300NS"
ATKK.DeviceDesc.DispName			= "Corega CG-WLUSB300NS"
TRENDnet.DeviceDesc					= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet.DeviceDesc.DispName		= "TRENDnet 150Mbps Micro Wireless N USB Adapter"
TRENDnet_2.DeviceDesc				= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
TRENDnet_2.DeviceDesc.DispName		= "TRENDnet 300Mbps Mini Wireless N USB Adapter"
Feixun.DeviceDesc 					= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
Feixun.DeviceDesc.DispName			= "FEIXUN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc 					= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
NetweeN.DeviceDesc.DispName			= "NetweeN Wireless LAN 802.11n USB 2.0 Network Adaptor"
XAVI.DeviceDesc 					= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI.DeviceDesc.DispName			= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Solo"
XAVI88cusc.DeviceDesc 				= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
XAVI88cusc.DeviceDesc.DispName		= "Realtek RTL8188CUS Wireless LAN 802.11n USB Slim Combo"
Netgear.DeviceDesc 					= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Netgear.DeviceDesc.DispName			= "NETGEAR WNA1000M N150 Wireless USB Micro Adapter"
Oar_Inc.DeviceDesc 					= "SW-WF02-AD15"
Oar_Inc.DeviceDesc.DispName			= "SW-WF02-AD15"
ASUS.DeviceDesc 					= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS.DeviceDesc.DispName			= "ASUS USB-N13 300Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc 					= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-2.DeviceDesc.DispName			= "ASUS USB-N10 150Mbps 11n Wireless USB dongle"
ASUS-17C0.DeviceDesc 				= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
ASUS-17C0.DeviceDesc.DispName		= "ASUS USB-N10E 150Mbps Wireless-N Adapter"
Hawking-1.DeviceDesc 				= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-1.DeviceDesc.DispName		= "Hawking HWDN3 Wls-N Dish Adapter"
Hawking-2.DeviceDesc 				= "Hawking HWUN4 Wls-300N Adapter"
Hawking-2.DeviceDesc.DispName		= "Hawking HWUN4 Wls-300N Adapter"
Compare-1.DeviceDesc 				= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
Compare-1.DeviceDesc.DispName		= "Compare Wireless LAN 802.11n USB 2.0 Network Adapter"
IO_DATA_094c.DeviceDesc				= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_094c.DeviceDesc.DispName	= "I-O DATA WN-G150UM Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc				= "I-O DATA WN-G300UA Wireless LAN Adapter"
IO_DATA_0950.DeviceDesc.DispName	= "I-O DATA WN-G300UA Wireless LAN Adapter"
TPLINK-0100.DeviceDesc				= "300Mbps Wireless High Power USB Adapter"
TPLINK-0100.DeviceDesc.DispName		= "300Mbps Wireless High Power USB Adapter"
Logitec_016D.DeviceDesc				= "Logitec LAN-WH300NU2 LAN Adapter"
Logitec_016D.DeviceDesc.DispName	= "Logitec LAN-WH300NU2 LAN Adapter"

;*******************************************************************************
; RTL8192DU Device description
;*******************************************************************************
RTL8192du.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192du0.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du0.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du1.DeviceDesc 				= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du1.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du2.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11N USB 2.0 Network Adapter MAC0"
RTL8192du2.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC0"
RTL8192du3.DeviceDesc           	= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
RTL8192du3.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11n USB 2.0 Network Adapter MAC1"
PCI_Abocom_du0.DeviceDesc 			= "GW-USDual300 MAC0"
PCI_Abocom_du0.DeviceDesc.DispName	= "GW-USDual300 MAC0"
PCI_Abocom_du1.DeviceDesc 			= "GW-USDual300 MAC1"
PCI_Abocom_du1.DeviceDesc.DispName	= "GW-USDual300 MAC1"
PCI_3_du0.DeviceDesc 				= "GW-USFang300 MAC0"
PCI_3_du0.DeviceDesc.DispName		= "GW-USFang300 MAC0"
PCI_3_du1.DeviceDesc 				= "GW-USFang300 MAC1"
PCI_3_du1.DeviceDesc.DispName		= "GW-USFang300 MAC1"
PCI_4_du0.DeviceDesc 				= "GW-USUltra300 MAC0"
PCI_4_du0.DeviceDesc.DispName		= "GW-USUltra300 MAC0"
PCI_4_du1.DeviceDesc 				= "GW-USUltra300 MAC1"
PCI_4_du1.DeviceDesc.DispName		= "GW-USUltra300 MAC1"
PCIWIDI_92DU.DeviceDesc 			= "MZK-WD300DH"
PCIWIDI_92DU.DeviceDesc.DispName	= "MZK-WD300DH"
Abocom_92DU0.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU0.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC0"
Abocom_92DU1.DeviceDesc				= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_92DU1.DeviceDesc.DispName	= "802.11 a/b/g/n Wireless LAN USB 2.0 Network Adapter MAC1"
Abocom_AB33.DeviceDesc				= "GW-300S KATANA"
Abocom_AB33.DeviceDesc.DispName		= "GW-300S KATANA"
Belkin-N600DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N600DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N450DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc			= "Belkin Wireless Adapter"
Belkin-N300DB.DeviceDesc.DispName	= "Belkin Wireless Adapter"
DLink-DWA151.DeviceDesc                 = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"   
DLink-DWA151.DeviceDesc.DispName        = "D-Link DWA-151 Wireless N 150 dual band USB Adapter"  
TRENDnet_3_du.DeviceDesc			= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
TRENDnet_3_du.DeviceDesc.DispName	= "TRENDnet 300Mbps Dual Band Wireless N USB Adapter"
Logitec.DeviceDesc					= "150N 5GHz USB Dongle"
Logitec.DeviceDesc.DispName			= "150N 5GHz USB Dongle"
EDIMAX5G.DeviceDesc			= "Realtek RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"
EDIMAX5G.DeviceDesc.DispName		= "Realtek RTL8192DU Wireless LAN 802.11a/n 5G USB 2.0 Network Adapter"
ScreenBeam.DeviceDesc 				= "Actiontec ScreenBeam USB Transmitter"
ScreenBeam.DeviceDesc.DispName		= "Actiontec ScreenBeam USB Transmitter"
;*******************************************************************************
; RTL8723au Device description
;*******************************************************************************
RTL8723au.DeviceDesc 				= "Realtek RTL8723AU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723au.DeviceDesc.DispName		= "Realtek RTL8723AU Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8723bu Device description
;*******************************************************************************
RTL8723bu.DeviceDesc 				= "Realtek RTL8723B Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8723bu.DeviceDesc.DispName		= "Realtek RTL8723B Wireless LAN 802.11n USB 2.0 Network Adapter"
;*******************************************************************************
; RTL8188EU Device description
;*******************************************************************************
RTL8188eu.DeviceDesc 				= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu.DeviceDesc.DispName		= "Realtek RTL8188EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188ee_vau.DeviceDesc 			= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
RTL8188ee_vau.DeviceDesc.DispName	= "Realtek RTL8188EE-VAU Wireless LAN 802.11n USB minicard"
RTL8188eu_0179.DeviceDesc 			= "Realtek RTL8188ETV Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8188eu_0179.DeviceDesc.DispName	= "Realtek RTL8188ETV Wireless LAN 802.11n USB 2.0 Network Adapter"
Abocom_8179.DeviceDesc 				= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
Abocom_8179.DeviceDesc.DispName		= "802.11n/b/g Mini Wireless LAN USB2.0 Adapter"
DLINK_330F.DeviceDesc 				= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_330F.DeviceDesc.DispName		= "D-Link DWA-125 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc 				= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3310.DeviceDesc.DispName		= "D-Link DWA-123 Wireless N 150 USB Adapter(rev.D)"
DLINK_3311.DeviceDesc 				= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
DLINK_3311.DeviceDesc.DispName		= "D-Link GO-USB-N150 Wireless N 150 Easy USB Adapter(rev.B)"
;*******************************************************************************
; RTL8812AU Device description
;*******************************************************************************
RTL8812au.DeviceDesc 					= "Realtek 8812AU Wireless LAN 802.11ac USB NIC"
RTL8812au.DeviceDesc.DispName			= "Realtek 8812AU Wireless LAN 802.11ac USB NIC"
RTL8812au_881A.DeviceDesc 				= "RTL8812AU-VS(802.11ac 2x2 USB2.0)"
RTL8812au_881A.DeviceDesc.DispName		= "RTL8812AU-VS(802.11ac 2x2 USB2.0)"
RTL8812au_881B.DeviceDesc 				= "RTL8812AU-VL(802.11ac 1x1 USB2.0)"
RTL8812au_881B.DeviceDesc.DispName		= "RTL8812AU-VL(802.11ac 1x1 USB2.0)"
RTL8812au_881C.DeviceDesc 				= "RTL8812AU-VN(802.11n 2x2 USB2.0)"
RTL8812au_881C.DeviceDesc.DispName		= "RTL8812AU-VN(802.11n 2x2 USB2.0)"

Belkin-AC950.DeviceDesc					= "Belkin USB Wireless Adapter"
Belkin-AC950.DeviceDesc.DispName		= "Belkin USB Wireless Adapter"

Netgear-A6200v2.DeviceDesc              = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"
Netgear-A6200v2.DeviceDesc.DispName     = "NETGEAR A6200V2 11AC Wireless USB 3.0 Adapter"

DLink-DWA183.DeviceDesc                 = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA183.DeviceDesc.DispName        = "D-Link DWA-183 Wireless AC Dual Band USB Adapter"
DLink-DWA182.DeviceDesc                 = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink-DWA182.DeviceDesc.DispName        = "D-Link DWA-182 Wireless AC Dual Band USB Adapter(rev.B)"
DLink_3315.DeviceDesc                	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3315.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc                 	= "Wireless AC1200 Dual Band USB Adapter"
DLink_3316.DeviceDesc.DispName        	= "Wireless AC1200 Dual Band USB Adapter"

Edimax_A822.DeviceDesc 				= "Edimax AC1200 Wireless LAN USB Adapter"
Edimax_A822.DeviceDesc.DispName		= "Edimax AC1200 Wireless LAN USB Adapter"

Sitecom_0074.DeviceDesc 				= "Sitecom WiFi USB adapter AC1200"
Sitecom_0074.DeviceDesc.DispName		= "Sitecom WiFi USB adapter AC1200"

Sitecom_007A.DeviceDesc 				= "WiFi High Gain USB Adapter AC600"
Sitecom_007A.DeviceDesc.DispName		= "WiFi High Gain USB Adapter AC600"

IO_DATA_0952.DeviceDesc					= "I-O DATA WN-AC867U Wireless LAN Adapter"
IO_DATA_0952.DeviceDesc.DispName		= "I-O DATA WN-AC867U Wireless LAN Adapter"
                                    	
Logitec_016E.DeviceDesc					= "Logitec AC866 Wireless USB Adapter"
Logitec_016E.DeviceDesc.DispName		= "Logitec AC866 Wireless USB Adapter"
                                    	
ASUS_17D2.DeviceDesc 					= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
ASUS_17D2.DeviceDesc.DispName			= "ASUS USB-AC56 802.11ac Wireless USB Adapter"
                                    	
Hawking_0022.DeviceDesc 				= "Hawking USB Wireless-AC Network Adapter"
Hawking_0022.DeviceDesc.DispName		= "Hawking USB Wireless-AC Network Adapter"

NEC_0408.DeviceDesc						= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"
NEC_0408.DeviceDesc.DispName			= "NEC AtermWL900U(PA-WL900U) Wireless Network Adapter"

Zyxel_3426.DeviceDesc					= "ZyXEL Wireless AC USB Adapter"
Zyxel_3426.DeviceDesc.DispName			= "ZyXEL Wireless AC USB Adapter"

WD_0632.DeviceDesc						= "WD My Net AC USB Adapter"
WD_0632.DeviceDesc.DispName				= "WD My Net AC USB Adapter"

EnGenius_0100.DeviceDesc				= "EnGenius 802.11ac Dual Band Wireless USB Adapter"
EnGenius_0100.DeviceDesc.DispName		= "EnGenius 802.11ac Dual Band Wireless USB Adapter"

Linksys_003F.DeviceDesc					= "Linksys WUSB6300"
Linksys_003F.DeviceDesc.DispName		= "Linksys WUSB6300"

Amped_9097.DeviceDesc					= "Amped Wireless ACA1 Wi-Fi Adapter"
Amped_9097.DeviceDesc.DispName			= "Amped Wireless ACA1 Wi-Fi Adapter"

TPLINK_0101.DeviceDesc					= "TP-LINK Wireless USB Adapter"
TPLINK_0101.DeviceDesc.DispName			= "TP-LINK Wireless USB Adapter"

PCI_AB30.DeviceDesc 				= "GW-900D"
PCI_AB30.DeviceDesc.DispName		= "GW-900D"

Abocom_8812.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_8812.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"

Abocom_0811.DeviceDesc 				= "802.11ac Wireless LAN Card"
Abocom_0811.DeviceDesc.DispName		= "802.11ac Wireless LAN Card"

TRENDnet_805B.DeviceDesc 			= "AC1200  Dual Band Wireless USB Adapter"
TRENDnet_805B.DeviceDesc.DispName		= "AC1200  Dual Band Wireless USB Adapter"

Buffalo_025D.DeviceDesc				= "BUFFALO WI-U3-866D Wireless LAN Adapter"
Buffalo_025D.DeviceDesc.DispName		= "BUFFALO WI-U3-866D Wireless LAN Adapter"

;*******************************************************************************
; RTL8811AU Device description
;*******************************************************************************
RTL8811au.DeviceDesc					= "Realtek RTL8811AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au.DeviceDesc.DispName			= "Realtek RTL8811AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au_Combo.DeviceDesc					= "Realtek RTL8821AU Wireless LAN 802.11ac USB 2.0 Network Adapter"
RTL8811au_Combo.DeviceDesc.DispName			= "Realtek RTL8821AU Wireless LAN 802.11ac USB 2.0 Network Adapter"

Buffalo-WI-U2-433DM.DeviceDesc 						= "BUFFALO WI-U2-433DM Wireless LAN Adapter"
Buffalo-WI-U2-433DM.DeviceDesc.DispName 		= "BUFFALO WI-U2-433DM Wireless LAN Adapter"

Edimax_AC600.DeviceDesc					= "Edimax AC600 Wireless LAN USB Adapter"
Edimax_AC600.DeviceDesc.DispName		= "Edimax AC600 Wireless LAN USB Adapter"

ELECOM_WDC433DU2.DeviceDesc				= "ELECOM WDC-433DU2H 11ac Wireless Adapter"
ELECOM_WDC433DU2.DeviceDesc.DispName	= "ELECOM WDC-433DU2H 11ac Wireless Adapter"

ELECOM_4009.DeviceDesc				= "ELECOM WDC-300SU2S Wireless Adapter"
ELECOM_4009.DeviceDesc.DispName		= "ELECOM WDC-300SU2S Wireless Adapter"

ELECOM_4008.DeviceDesc				= "ELECOM WDC-150SU2M Wireless Adapter"
ELECOM_4008.DeviceDesc.DispName		= "ELECOM WDC-150SU2M Wireless Adapter"

Hawking_0023.DeviceDesc					= "Hawking USB WLS 11AC Adapter"
Hawking_0023.DeviceDesc.DispName		= "Hawking USB WLS 11AC Adapter"

IO_DATA_AC433UA.DeviceDesc					= "I-O DATA WN-AC433UA Wireless LAN Adapter"
IO_DATA_AC433UA.DeviceDesc.DispName		= "I-O DATA WN-AC433UA Wireless LAN Adapter"

DLink-DWA171.DeviceDesc	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink-DWA171.DeviceDesc.DispName	=	 "D-Link DWA-171 Wireless AC Dual Band Adapter"
DLink_3318.DeviceDesc	=	 "Wireless AC600 Dual Band High-Gain USB Adapter"
DLink_3318.DeviceDesc.DispName	=	 "Wireless AC600 Dual Band High-Gain USB Adapter"

TRENDnet_804B.DeviceDesc	=	 "AC600 Dual Band Wireless USB Adapter"
TRENDnet_804B.DeviceDesc.DispName	=	 "AC600 Dual Band Wireless USB Adapter"

PCI_AB32.DeviceDesc					=	"GW-450S"
PCI_AB32.DeviceDesc.DispName		=	"GW-450S"

IO_DATA_0959.DeviceDesc					=	"I-O DATA WN-AC433UM Wireless LAN Adapter"
IO_DATA_0959.DeviceDesc.DispName		=	"I-O DATA WN-AC433UM Wireless LAN Adapter"
;*******************************************************************************
; RTL8192E Device description
;*******************************************************************************
RTL8192eu.DeviceDesc					= "Realtek RTL8192EU Wireless LAN 802.11n USB 2.0 Network Adapter"
RTL8192eu.DeviceDesc.DispName			= "Realtek RTL8192EU Wireless LAN 802.11n USB 2.0 Network Adapter"
DLink_2001.DeviceDesc					= "D-Link DWA-131 Wireless N Nano USB Adapter"
DLink_2001.DeviceDesc.DispName			= "D-Link DWA-131 Wireless N Nano USB Adapter"

;*******************************************************************************
; RTL8814AU Device description
;*******************************************************************************
RTL8814au.DeviceDesc 					= "Realtek 8814AU Wireless LAN 802.11ac USB NIC"
RTL8814au.DeviceDesc.DispName			= "Realtek 8814AU Wireless LAN 802.11ac USB NIC"

;*******************************************************************************
; RTL8821BU Device description
;*******************************************************************************
RTL8821bu.DeviceDesc 					= "Realtek 8821BU Wireless LAN 802.11ac USB NIC"
RTL8821bu.DeviceDesc.DispName			= "Realtek 8821BU Wireless LAN 802.11ac USB NIC"
