;****************************************************************
; ASIX AX88772/772A USB2.0 to Fast Ethernet Adapter
;
; Copyright 2003-2008, ASIX Electronics Corporation
;
; Version: 3.8.3.14	for windows vista
;****************************************************************
[Version]
Signature  = "$Windows NT$"
CatalogFile = ax88772ex.cat
Class      = Net
ClassGUID  = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider   = %ASIX%
DriverVer = 11/18/2008, 3.8.3.14

[Manufacturer]
%ASIX%   = USB

[ControlFlags]
ExcludeFromSelect = USB\VID_0B95&PID_7720, USB\VID_0B95&PID_772A, USB\VID_0DB0&PID_A877

[USB]
%AX88772.DeviceDesc% = AX88772.Ndi,USB\VID_0B95&PID_7720
%AX88772A.DeviceDesc% = AX88772A.Ndi,USB\VID_0B95&PID_772A
%MSI.DeviceDesc% = AX88772A.Ndi,USB\VID_0DB0&PID_A877

;****************************************************************
[AX88772.Ndi]
AddReg          = AX88772.NT.Reg, AX88772.Con.Reg
Characteristics = 0x84
BusType         = 15
CopyFiles       = CopyFile.Sys
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[AX88772.Ndi.Services]
AddService = AX88772, 2, AX88772.Service, Common.EventLog

[AX88772A.Ndi]
AddReg          = AX88772.NT.Reg, AX88772A.Con.Reg
Characteristics = 0x84
BusType         = 15
CopyFiles       = CopyFile.Sys
*IfType         = 6		; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0		; NdisMedium802_3
*PhysicalMediaType = 14		; NdisPhysicalMedium802_3

[AX88772A.Ndi.Services]
AddService = AX88772, 2, AX88772.Service, Common.EventLog

;****************************************************************
; Driver parameters
;****************************************************************
[AX88772.Con.Reg]
HKR, ,               ChipCode,   0, "0"

; Connection Type
HKR,Ndi\params\*SpeedDuplex,ParamDesc,,%ConnectionType%
HKR,Ndi\params\*SpeedDuplex,default,,"0"
HKR,Ndi\params\*SpeedDuplex,type,,"enum"
HKR,Ndi\params\*SpeedDuplex\enum,0,,%AutoSense%
HKR,Ndi\params\*SpeedDuplex\enum,1,,%10Half%
HKR,Ndi\params\*SpeedDuplex\enum,2,,%10Full%
HKR,Ndi\params\*SpeedDuplex\enum,3,,%100Half%
HKR,Ndi\params\*SpeedDuplex\enum,4,,%100Full%

; Mac Address
HKR,Ndi\params\NetworkAddress,ParamDesc,0,%NetworkAddress%
HKR,Ndi\params\NetworkAddress,type,0,"edit"
HKR,Ndi\params\NetworkAddress,default,0, "000000000000"
HKR,Ndi\params\NetworkAddress,LimitText,0,"12"
HKR,Ndi\params\NetworkAddress,UpperCase,0,"1"
HKR,Ndi\params\NetworkAddress,Optional,0,"1"

; Flow Control
HKR,Ndi\params\*FlowControl,ParamDesc,,%FlowControl%
HKR,Ndi\params\*FlowControl,default,,"3"
HKR,Ndi\params\*FlowControl,type,,"enum"
HKR,Ndi\params\*FlowControl\enum,0,,%Disable%
HKR,Ndi\params\*FlowControl\enum,1,,%TxEnable%
HKR,Ndi\params\*FlowControl\enum,2,,%RxEnable%
HKR,Ndi\params\*FlowControl\enum,3,,%AllEnable%

; Wake Up
HKR,Ndi\params\WakeUp,ParamDesc,,%WakeUp%
HKR,Ndi\params\WakeUp,default,,"0"
HKR,Ndi\params\WakeUp,type,,"enum"
HKR,Ndi\params\WakeUp\enum,0,,%Disable%
HKR,Ndi\params\WakeUp\enum,2,,%LinkUp%
HKR,Ndi\params\WakeUp\enum,4,,%MagicPacket%
HKR,Ndi\params\WakeUp\enum,6,,%Both%

; Qos Packet Tagging
HKR,Ndi\params\QosTag,ParamDesc,,%QoSTagging%
HKR,Ndi\params\QosTag,default,,"0"
HKR,Ndi\params\QosTag,type,,"enum"
HKR,Ndi\params\QosTag\enum,0,,%Disable%
HKR,Ndi\params\QosTag\enum,1,,%Enable%

[AX88772A.Con.Reg]
HKR, ,               ChipCode,   0, "1"

; Connection Type
HKR,Ndi\params\*SpeedDuplex,ParamDesc,,%ConnectionType%
HKR,Ndi\params\*SpeedDuplex,default,,"0"
HKR,Ndi\params\*SpeedDuplex,type,,"enum"
HKR,Ndi\params\*SpeedDuplex\enum,0,,%AutoSense%
HKR,Ndi\params\*SpeedDuplex\enum,1,,%10Half%
HKR,Ndi\params\*SpeedDuplex\enum,2,,%10Full%
HKR,Ndi\params\*SpeedDuplex\enum,3,,%100Half%
HKR,Ndi\params\*SpeedDuplex\enum,4,,%100Full%

; Mac Address
HKR,Ndi\params\NetworkAddress,ParamDesc,0,%NetworkAddress%
HKR,Ndi\params\NetworkAddress,type,0,"edit"
HKR,Ndi\params\NetworkAddress,default,0, "000000000000"
HKR,Ndi\params\NetworkAddress,LimitText,0,"12"
HKR,Ndi\params\NetworkAddress,UpperCase,0,"1"
HKR,Ndi\params\NetworkAddress,Optional,0,"1"

; Flow Control
HKR,Ndi\params\*FlowControl,ParamDesc,,%FlowControl%
HKR,Ndi\params\*FlowControl,default,,"3"
HKR,Ndi\params\*FlowControl,type,,"enum"
HKR,Ndi\params\*FlowControl\enum,0,,%Disable%
HKR,Ndi\params\*FlowControl\enum,1,,%TxEnable%
HKR,Ndi\params\*FlowControl\enum,2,,%RxEnable%
HKR,Ndi\params\*FlowControl\enum,3,,%AllEnable%

; Wake Up
HKR,Ndi\params\WakeUp,ParamDesc,,%WakeUp%
HKR,Ndi\params\WakeUp,default,,"0"
HKR,Ndi\params\WakeUp,type,,"enum"
HKR,Ndi\params\WakeUp\enum,0,,%Disable%
HKR,Ndi\params\WakeUp\enum,2,,%LinkUp%
HKR,Ndi\params\WakeUp\enum,4,,%MagicPacket%
HKR,Ndi\params\WakeUp\enum,8,,%WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,6,,%LinkUp-MagicPacket%
HKR,Ndi\params\WakeUp\enum,10,,%LinkUp-WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,12,,%MagicPacket-WakeUpFrame%
HKR,Ndi\params\WakeUp\enum,14,,%All%

;Wake Up Frame
HKR,Ndi\params\WakeUpFrameType,ParamDesc,,%WakeUpFrameType%
HKR,Ndi\params\WakeUpFrameType,default,,"0"
HKR,Ndi\params\WakeUpFrameType,type,,"enum"
HKR,Ndi\params\WakeUpFrameType\enum,0,,%WindowsDefault%
HKR,Ndi\params\WakeUpFrameType\enum,1,,%PING%
HKR,Ndi\params\WakeUpFrameType\enum,2,,%ARP%
HKR,Ndi\params\WakeUpFrameType\enum,3,,%PING-ARP%

; Qos Packet Tagging
HKR,Ndi\params\QosTag,ParamDesc,,%QoSTagging%
HKR,Ndi\params\QosTag,default,,"0"
HKR,Ndi\params\QosTag,type,,"enum"
HKR,Ndi\params\QosTag\enum,0,,%Disable%
HKR,Ndi\params\QosTag\enum,1,,%Enable%

;VLAN ID
HKR, Ndi\Params\VLAN_ID,  ParamDesc,  , %VLANID%
HKR, Ndi\Params\VLAN_ID,  Type,       , "int"
HKR, Ndi\Params\VLAN_ID,  Default,    , "0"
HKR, Ndi\params\VLAN_ID,  min,        , "0"
HKR, Ndi\params\VLAN_ID,  max,        , "4095"
HKR, Ndi\params\VLAN_ID,  step,       , "1"
HKR, NDI\params\VLAN_ID,  UpperCase,  , "1"
HKR, NDI\params\VLAN_ID,  optional,   , "1"

;****************************************************************
; Install section for Windows NT 5
;****************************************************************
[AX88772.NT.Reg]
; Interfaces
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi,            Service,    0, "AX88772"

HKR,,LogErrorMessages, 0, "1"

[AX88772.Service]
DisplayName    = %AX88772.DeviceDesc%
ServiceType    = 1
StartType      = 3
ErrorControl   = 1
ServiceBinary  = %12%\ax88772.sys
LoadOrderGroup = NDIS

[Common.EventLog]
AddReg = Common.AddEventLog.Reg

[Common.AddEventLog.Reg]
HKR, , EventMessageFile, 0x00020000,"%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\system32\drivers\ax88772.sys"
HKR, , TypesSupported  , 0x00010001, 7

[CopyFile.Sys]
ax88772.sys,,,2

;**********************************************************************
; Destination directories
;**********************************************************************
[DestinationDirs]
CopyFile.Sys	= 12

[SourceDisksNames]
1=%AX88772.DiskName%,,

[SourceDisksFiles]
ax88772.sys=1,,ax88772.sys,10000

;**********************************************************************
; Localizable strings
;**********************************************************************
[Strings]
ASIX = "ASIX"
AX88772.DiskName = "USB2.0 to Fast Ethernet Driver Diskette"
AX88772.DeviceDesc = "ASIX AX88772 USB2.0 to Fast Ethernet Adapter"
AX88772A.DeviceDesc = "ASIX AX88772A USB2.0 to Fast Ethernet Adapter"
MSI.DeviceDesc = "MSI USB Network Controller"
AX88772.DisplayName = "USB2.0 to Fast Ethernet Adapter"

ConnectionType         = "Connection Type"
AutoSense              = "AutoSense"
10Half                 = "10BaseT Half_Duplex"
10Full                 = "10BaseT Full_Duplex"
100Half                = "100BaseTx Half_Duplex"
100Full                = "100BaseTx Full_Duplex"
NetworkAddress         = "NetworkAddress"
FlowControl            = "Flow Control"
Disable                = "Disable"
Enable                 = "Enable"
TxEnable               = "Tx Enable"
RxEnable               = "Rx Enable"
AllEnable              = "Rx & Tx Enable"
WakeUp                 = "Wake Up"
LinkUp                 = "Link Up"
MagicPacket            = "Magic Packet"
WakeUpFrame            = "Wake-Up Frame"
LinkUp-MagicPacket     = "Link Up/Magic Packet"
LinkUp-WakeUpFrame     = "Link Up/Wake-Up Frame"
MagicPacket-WakeUpFrame= "Magic Packet/Wake-Up Frame"
All                    = "All"
Both                   = "Both"
QoSTagging             = "QoS Packet Tagging"
WakeUpFrameType        = "Wake-Up Frame Type"
WindowsDefault         = "Windows Default"
PING                   = "PING"
ARP                    = "ARP"
PING-ARP               = "PING/ARP"
VLANID                 = "VLAN ID"
