## Path:	Hardware/IDE
## Description:	IDE device settings
## Type:	string
## Default:	""
#
# Force DMA mode for selected device. Use pairs <device>:<dma_mode> separated
# by space - dma_mode can be "on" (enable default DMA mode), "off" (disable DMA
# mode) or any mode supported by hdparm (e.g. "mdma2", "udma5", ...)
# Example: "/dev/hdc:off /dev/hdd:udma2"
#
DEVICES_FORCE_IDE_DMA="/dev/hde:udma5 /dev/hdg:udma5"
